Frame 1 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.579004000
    Time delta from previous packet: 0.000000000 seconds
    Time since reference or first frame: 0.000000000 seconds
    Frame Number: 1
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x20 (DSCP 0x08: Class Selector 1; ECN: 0x00)
        0010 00.. = Differentiated Services Codepoint: Class Selector 1 (0x08)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x0a39 (2617)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xddc7 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 0, Ack: 0, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0xb2c4 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

Frame 2 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.579031000
    Time delta from previous packet: 0.000027000 seconds
    Time since reference or first frame: 0.000027000 seconds
    Frame Number: 2
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x5243 (21059)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x51dd)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 0, Ack: 1, Len: 0
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x3726 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 1
        The RTT to ACK the segment was: 0.000027000 seconds

Frame 3 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.618391000
    Time delta from previous packet: 0.039360000 seconds
    Time since reference or first frame: 0.039387000 seconds
    Frame Number: 3
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb6cd (46797)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2d5b (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x92ea (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 2
        The RTT to ACK the segment was: 0.039360000 seconds

Frame 4 (646 bytes on wire, 646 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.637854000
    Time delta from previous packet: 0.019463000 seconds
    Time since reference or first frame: 0.058850000 seconds
    Frame Number: 4
    Packet Length: 646 bytes
    Capture Length: 646 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 632
    Identification: 0xb6ce (46798)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2b0a (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 592
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 1
    Next sequence number: 593
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xde70 (correct)
Hypertext Transfer Protocol
    POST /servlet/InstallNotify HTTP/1.1\r\n
        Request Method: POST
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Host: 195.235.160.80:8080\r\n
    accept: */*,*/*\r\n
    accept-charset: utf-8,*\r\n
    accept-encoding: deflate\r\n
    accept-language: es\r\n
    Content-Length: 11\r\n
    content-type: text/plain\r\n
    Date: Wed, 20 Dec 2006 13:44:12\r\n
    user-agent: MOT-Z3/08.01.05R MIB/BER2.2 Profile/MIDP-2.0 Configuration/CLDC-1.1 EGE/1.0 UP.Link/6.3.1.14.0\r\n
    x-wap-profile: "http://motorola.handango.com/phoneconfig/z3/Profile/z3.rdf"\r\n
    x-up-forwarded-for: 10.146.15.59\r\n
    x-up-subscriber-coi: coiwap\r\n
    Via: 1.1 mbe-proxy6pe.wap.oleada.com:8080\r\n
    \r\n

Frame 5 (1010 bytes on wire, 1010 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.641927000
    Time delta from previous packet: 0.004073000 seconds
    Time since reference or first frame: 0.062923000 seconds
    Frame Number: 5
    Packet Length: 1010 bytes
    Capture Length: 1010 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 996
    Identification: 0x5244 (21060)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4e28)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 1, Ack: 593, Len: 956
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 1
    Next sequence number: 957
    Acknowledgement number: 593
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16928
    Checksum: 0x5a7e (incorrect, should be 0x4060)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 4
        The RTT to ACK the segment was: 0.004073000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 404 /servlet/InstallNotify\r\n
        Response Code: 404
    Content-Type: text/html;charset=ISO-8859-1\r\n
    Content-Language: es-ES\r\n
    Transfer-Encoding: chunked\r\n
    Date: Wed, 20 Dec 2006 12:44:32 GMT\r\n
    Server: Apache-Coyote/1.1\r\n
    \r\n
    Data (756 bytes)

0000  32 65 64 0d 0a 3c 68 74 6d 6c 3e 3c 68 65 61 64   2ed..<html><head
0010  3e 3c 74 69 74 6c 65 3e 41 70 61 63 68 65 20 54   ><title>Apache T
0020  6f 6d 63 61 74 2f 34 2e 31 2e 32 39 2d 4c 45 2d   omcat/4.1.29-LE-
0030  6a 64 6b 31 34 20 2d 20 45 72 72 6f 72 20 72 65   jdk14 - Error re
0040  70 6f 72 74 3c 2f 74 69 74 6c 65 3e 3c 53 54 59   port</title><STY
0050  4c 45 3e 3c 21 2d 2d 48 31 7b 66 6f 6e 74 2d 66   LE><!--H1{font-f
0060  61 6d 69 6c 79 20 3a 20 73 61 6e 73 2d 73 65 72   amily : sans-ser
0070  69 66 2c 41 72 69 61 6c 2c 54 61 68 6f 6d 61 3b   if,Arial,Tahoma;
0080  63 6f 6c 6f 72 20 3a 20 77 68 69 74 65 3b 62 61   color : white;ba
0090  63 6b 67 72 6f 75 6e 64 2d 63 6f 6c 6f 72 20 3a   ckground-color :
00a0  20 23 30 30 38 36 62 32 3b 7d 20 48 33 7b 66 6f    #0086b2;} H3{fo
00b0  6e 74 2d 66 61 6d 69 6c 79 20 3a 20 73 61 6e 73   nt-family : sans
00c0  2d 73 65 72 69 66 2c 41 72 69 61 6c 2c 54 61 68   -serif,Arial,Tah
00d0  6f 6d 61 3b 63 6f 6c 6f 72 20 3a 20 77 68 69 74   oma;color : whit
00e0  65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f 6c   e;background-col
00f0  6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20 42   or : #0086b2;} B
0100  4f 44 59 7b 66 6f 6e 74 2d 66 61 6d 69 6c 79 20   ODY{font-family 
0110  3a 20 73 61 6e 73 2d 73 65 72 69 66 2c 41 72 69   : sans-serif,Ari
0120  61 6c 2c 54 61 68 6f 6d 61 3b 63 6f 6c 6f 72 20   al,Tahoma;color 
0130  3a 20 62 6c 61 63 6b 3b 62 61 63 6b 67 72 6f 75   : black;backgrou
0140  6e 64 2d 63 6f 6c 6f 72 20 3a 20 77 68 69 74 65   nd-color : white
0150  3b 7d 20 42 7b 63 6f 6c 6f 72 20 3a 20 77 68 69   ;} B{color : whi
0160  74 65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f   te;background-co
0170  6c 6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20   lor : #0086b2;} 
0180  48 52 7b 63 6f 6c 6f 72 20 3a 20 23 30 30 38 36   HR{color : #0086
0190  62 32 3b 7d 20 2d 2d 3e 3c 2f 53 54 59 4c 45 3e   b2;} --></STYLE>
01a0  20 3c 2f 68 65 61 64 3e 3c 62 6f 64 79 3e 3c 68    </head><body><h
01b0  31 3e 48 54 54 50 20 53 74 61 74 75 73 20 34 30   1>HTTP Status 40
01c0  34 20 2d 20 2f 73 65 72 76 6c 65 74 2f 49 6e 73   4 - /servlet/Ins
01d0  74 61 6c 6c 4e 6f 74 69 66 79 3c 2f 68 31 3e 3c   tallNotify</h1><
01e0  48 52 20 73 69 7a 65 3d 22 31 22 20 6e 6f 73 68   HR size="1" nosh
01f0  61 64 65 3e 3c 70 3e 3c 62 3e 74 79 70 65 3c 2f   ade><p><b>type</
0200  62 3e 20 53 74 61 74 75 73 20 72 65 70 6f 72 74   b> Status report
0210  3c 2f 70 3e 3c 70 3e 3c 62 3e 6d 65 73 73 61 67   </p><p><b>messag
0220  65 3c 2f 62 3e 20 3c 75 3e 2f 73 65 72 76 6c 65   e</b> <u>/servle
0230  74 2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 3c   t/InstallNotify<
0240  2f 75 3e 3c 2f 70 3e 3c 70 3e 3c 62 3e 64 65 73   /u></p><p><b>des
0250  63 72 69 70 74 69 6f 6e 3c 2f 62 3e 20 3c 75 3e   cription</b> <u>
0260  54 68 65 20 72 65 71 75 65 73 74 65 64 20 72 65   The requested re
0270  73 6f 75 72 63 65 20 28 2f 73 65 72 76 6c 65 74   source (/servlet
0280  2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 29 20   /InstallNotify) 
0290  69 73 20 6e 6f 74 20 61 76 61 69 6c 61 62 6c 65   is not available
02a0  2e 3c 2f 75 3e 3c 2f 70 3e 3c 48 52 20 73 69 7a   .</u></p><HR siz
02b0  65 3d 22 31 22 20 6e 6f 73 68 61 64 65 3e 3c 68   e="1" noshade><h
02c0  33 3e 41 70 61 63 68 65 20 54 6f 6d 63 61 74 2f   3>Apache Tomcat/
02d0  34 2e 31 2e 32 39 2d 4c 45 2d 6a 64 6b 31 34 3c   4.1.29-LE-jdk14<
02e0  2f 68 33 3e 3c 2f 62 6f 64 79 3e 3c 2f 68 74 6d   /h3></body></htm
02f0  6c 3e 0d 0a                                       l>..

Frame 6 (59 bytes on wire, 59 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.641966000
    Time delta from previous packet: 0.000039000 seconds
    Time since reference or first frame: 0.062962000 seconds
    Frame Number: 6
    Packet Length: 59 bytes
    Capture Length: 59 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 45
    Identification: 0x5245 (21061)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x51de)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 957, Ack: 593, Len: 5
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 957
    Next sequence number: 962
    Acknowledgement number: 593
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16928
    Checksum: 0x56c7 (incorrect, should be 0x1c07)
Hypertext Transfer Protocol
    Data (5 bytes)

0000  30 0d 0a 0d 0a                                    0....

Frame 7 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.642711000
    Time delta from previous packet: 0.000745000 seconds
    Time since reference or first frame: 0.063707000 seconds
    Frame Number: 7
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb6cf (46799)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2d59 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 593, Ack: 957, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 593
    Acknowledgement number: 957
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x882a (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 5
        The RTT to ACK the segment was: 0.000784000 seconds

Frame 8 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.642720000
    Time delta from previous packet: 0.000009000 seconds
    Time since reference or first frame: 0.063716000 seconds
    Frame Number: 8
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb6d0 (46800)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2d58 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 593, Ack: 962, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 593
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x8825 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 6
        The RTT to ACK the segment was: 0.000754000 seconds

Frame 9 (65 bytes on wire, 65 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.647572000
    Time delta from previous packet: 0.004852000 seconds
    Time since reference or first frame: 0.068568000 seconds
    Frame Number: 9
    Packet Length: 65 bytes
    Capture Length: 65 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 51
    Identification: 0xb6d1 (46801)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2d4c (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 593, Ack: 962, Len: 11
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 593
    Next sequence number: 604
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x8f75 (correct)
Hypertext Transfer Protocol
    Data (11 bytes)

0000  39 30 30 20 53 75 63 63 65 73 73                  900 Success

Frame 10 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.816770000
    Time delta from previous packet: 0.169198000 seconds
    Time since reference or first frame: 0.237766000 seconds
    Frame Number: 10
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x5246 (21062)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x51e2)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 962, Ack: 604, Len: 0
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 962
    Acknowledgement number: 604
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16917
    Checksum: 0x56c2 (incorrect, should be 0x6029)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 9
        The RTT to ACK the segment was: 0.169198000 seconds

Frame 11 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.828018000
    Time delta from previous packet: 0.011248000 seconds
    Time since reference or first frame: 0.249014000 seconds
    Frame Number: 11
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb6d2 (46802)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2d56 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 604, Ack: 962, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 604
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6692
    Checksum: 0x8819 (correct)

Frame 12 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.828039000
    Time delta from previous packet: 0.000021000 seconds
    Time since reference or first frame: 0.249035000 seconds
    Frame Number: 12
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x5247 (21063)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x51e1)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 962, Ack: 605, Len: 0
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 962
    Acknowledgement number: 605
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16917
    Checksum: 0x56c2 (incorrect, should be 0x6028)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 11
        The RTT to ACK the segment was: 0.000021000 seconds

Frame 13 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.828202000
    Time delta from previous packet: 0.000163000 seconds
    Time since reference or first frame: 0.249198000 seconds
    Frame Number: 13
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x5248 (21064)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x51e0)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 30297 (30297), Seq: 962, Ack: 605, Len: 0
    Source port: 8080 (8080)
    Destination port: 30297 (30297)
    Sequence number: 962
    Acknowledgement number: 605
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16917
    Checksum: 0x56c2 (incorrect, should be 0x6027)

Frame 14 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:44:32.828748000
    Time delta from previous packet: 0.000546000 seconds
    Time since reference or first frame: 0.249744000 seconds
    Frame Number: 14
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb47f (46207)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2fa9 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 30297 (30297), Dst Port: 8080 (8080), Seq: 605, Ack: 963, Len: 0
    Source port: 30297 (30297)
    Destination port: 8080 (8080)
    Sequence number: 605
    Acknowledgement number: 963
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x8818 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 13
        The RTT to ACK the segment was: 0.000546000 seconds

Frame 15 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.043243000
    Time delta from previous packet: 45.214495000 seconds
    Time since reference or first frame: 45.464239000 seconds
    Frame Number: 15
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x20 (DSCP 0x08: Class Selector 1; ECN: 0x00)
        0010 00.. = Differentiated Services Codepoint: Class Selector 1 (0x08)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x3be9 (15337)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xac17 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 0, Ack: 0, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x2e8c (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

Frame 16 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.043280000
    Time delta from previous packet: 0.000037000 seconds
    Time since reference or first frame: 45.464276000 seconds
    Frame Number: 16
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x546a (21610)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4fb6)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 34094 (34094), Seq: 0, Ack: 1, Len: 0
    Source port: 8080 (8080)
    Destination port: 34094 (34094)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0xfb69 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 15
        The RTT to ACK the segment was: 0.000037000 seconds

Frame 17 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.096013000
    Time delta from previous packet: 0.052733000 seconds
    Time since reference or first frame: 45.517009000 seconds
    Frame Number: 17
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe1e6 (57830)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x0242 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x572e (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 16
        The RTT to ACK the segment was: 0.052733000 seconds

Frame 18 (657 bytes on wire, 657 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.099177000
    Time delta from previous packet: 0.003164000 seconds
    Time since reference or first frame: 45.520173000 seconds
    Frame Number: 18
    Packet Length: 657 bytes
    Capture Length: 657 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 643
    Identification: 0xe1e7 (57831)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xffe5 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 603
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 1
    Next sequence number: 604
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xa408 (correct)
Hypertext Transfer Protocol
    POST /servlet/InstallNotify HTTP/1.1\r\n
        Request Method: POST
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Host: 195.235.160.80:8080\r\n
    accept: */*,*/*\r\n
    accept-charset: utf-8,*\r\n
    accept-encoding: deflate\r\n
    accept-language: es\r\n
    Content-Length: 11\r\n
    content-type: text/plain\r\n
    Date: Wed, 20 Dec 2006 13:44:58\r\n
    user-agent: MOT-Z3/08.01.05R MIB/BER2.2 Profile/MIDP-2.0 Configuration/CLDC-1.1 EGE/1.0 UP.Link/6.3.1.14.0\r\n
    x-wap-profile: "http://motorola.handango.com/phoneconfig/z3/Profile/z3.rdf"\r\n
    x-up-forwarded-for: 10.146.15.59\r\n
    x-up-subscriber-coi: coiwap\r\n
    Via: 1.1 mbe-proxy6pe.wap.oleada.com:8080\r\n
    \r\n
    Data (11 bytes)

0000  39 30 30 20 53 75 63 63 65 73 73                  900 Success

Frame 19 (1010 bytes on wire, 1010 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.102891000
    Time delta from previous packet: 0.003714000 seconds
    Time since reference or first frame: 45.523887000 seconds
    Frame Number: 19
    Packet Length: 1010 bytes
    Capture Length: 1010 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 996
    Identification: 0x5471 (21617)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4bfb)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 34094 (34094), Seq: 1, Ack: 604, Len: 956
    Source port: 8080 (8080)
    Destination port: 34094 (34094)
    Sequence number: 1
    Next sequence number: 957
    Acknowledgement number: 604
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16917
    Checksum: 0x5a7e (incorrect, should be 0xfea4)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 18
        The RTT to ACK the segment was: 0.003714000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 404 /servlet/InstallNotify\r\n
        Response Code: 404
    Content-Type: text/html;charset=ISO-8859-1\r\n
    Content-Language: es-ES\r\n
    Transfer-Encoding: chunked\r\n
    Date: Wed, 20 Dec 2006 12:45:18 GMT\r\n
    Server: Apache-Coyote/1.1\r\n
    \r\n
    Data (756 bytes)

0000  32 65 64 0d 0a 3c 68 74 6d 6c 3e 3c 68 65 61 64   2ed..<html><head
0010  3e 3c 74 69 74 6c 65 3e 41 70 61 63 68 65 20 54   ><title>Apache T
0020  6f 6d 63 61 74 2f 34 2e 31 2e 32 39 2d 4c 45 2d   omcat/4.1.29-LE-
0030  6a 64 6b 31 34 20 2d 20 45 72 72 6f 72 20 72 65   jdk14 - Error re
0040  70 6f 72 74 3c 2f 74 69 74 6c 65 3e 3c 53 54 59   port</title><STY
0050  4c 45 3e 3c 21 2d 2d 48 31 7b 66 6f 6e 74 2d 66   LE><!--H1{font-f
0060  61 6d 69 6c 79 20 3a 20 73 61 6e 73 2d 73 65 72   amily : sans-ser
0070  69 66 2c 41 72 69 61 6c 2c 54 61 68 6f 6d 61 3b   if,Arial,Tahoma;
0080  63 6f 6c 6f 72 20 3a 20 77 68 69 74 65 3b 62 61   color : white;ba
0090  63 6b 67 72 6f 75 6e 64 2d 63 6f 6c 6f 72 20 3a   ckground-color :
00a0  20 23 30 30 38 36 62 32 3b 7d 20 48 33 7b 66 6f    #0086b2;} H3{fo
00b0  6e 74 2d 66 61 6d 69 6c 79 20 3a 20 73 61 6e 73   nt-family : sans
00c0  2d 73 65 72 69 66 2c 41 72 69 61 6c 2c 54 61 68   -serif,Arial,Tah
00d0  6f 6d 61 3b 63 6f 6c 6f 72 20 3a 20 77 68 69 74   oma;color : whit
00e0  65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f 6c   e;background-col
00f0  6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20 42   or : #0086b2;} B
0100  4f 44 59 7b 66 6f 6e 74 2d 66 61 6d 69 6c 79 20   ODY{font-family 
0110  3a 20 73 61 6e 73 2d 73 65 72 69 66 2c 41 72 69   : sans-serif,Ari
0120  61 6c 2c 54 61 68 6f 6d 61 3b 63 6f 6c 6f 72 20   al,Tahoma;color 
0130  3a 20 62 6c 61 63 6b 3b 62 61 63 6b 67 72 6f 75   : black;backgrou
0140  6e 64 2d 63 6f 6c 6f 72 20 3a 20 77 68 69 74 65   nd-color : white
0150  3b 7d 20 42 7b 63 6f 6c 6f 72 20 3a 20 77 68 69   ;} B{color : whi
0160  74 65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f   te;background-co
0170  6c 6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20   lor : #0086b2;} 
0180  48 52 7b 63 6f 6c 6f 72 20 3a 20 23 30 30 38 36   HR{color : #0086
0190  62 32 3b 7d 20 2d 2d 3e 3c 2f 53 54 59 4c 45 3e   b2;} --></STYLE>
01a0  20 3c 2f 68 65 61 64 3e 3c 62 6f 64 79 3e 3c 68    </head><body><h
01b0  31 3e 48 54 54 50 20 53 74 61 74 75 73 20 34 30   1>HTTP Status 40
01c0  34 20 2d 20 2f 73 65 72 76 6c 65 74 2f 49 6e 73   4 - /servlet/Ins
01d0  74 61 6c 6c 4e 6f 74 69 66 79 3c 2f 68 31 3e 3c   tallNotify</h1><
01e0  48 52 20 73 69 7a 65 3d 22 31 22 20 6e 6f 73 68   HR size="1" nosh
01f0  61 64 65 3e 3c 70 3e 3c 62 3e 74 79 70 65 3c 2f   ade><p><b>type</
0200  62 3e 20 53 74 61 74 75 73 20 72 65 70 6f 72 74   b> Status report
0210  3c 2f 70 3e 3c 70 3e 3c 62 3e 6d 65 73 73 61 67   </p><p><b>messag
0220  65 3c 2f 62 3e 20 3c 75 3e 2f 73 65 72 76 6c 65   e</b> <u>/servle
0230  74 2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 3c   t/InstallNotify<
0240  2f 75 3e 3c 2f 70 3e 3c 70 3e 3c 62 3e 64 65 73   /u></p><p><b>des
0250  63 72 69 70 74 69 6f 6e 3c 2f 62 3e 20 3c 75 3e   cription</b> <u>
0260  54 68 65 20 72 65 71 75 65 73 74 65 64 20 72 65   The requested re
0270  73 6f 75 72 63 65 20 28 2f 73 65 72 76 6c 65 74   source (/servlet
0280  2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 29 20   /InstallNotify) 
0290  69 73 20 6e 6f 74 20 61 76 61 69 6c 61 62 6c 65   is not available
02a0  2e 3c 2f 75 3e 3c 2f 70 3e 3c 48 52 20 73 69 7a   .</u></p><HR siz
02b0  65 3d 22 31 22 20 6e 6f 73 68 61 64 65 3e 3c 68   e="1" noshade><h
02c0  33 3e 41 70 61 63 68 65 20 54 6f 6d 63 61 74 2f   3>Apache Tomcat/
02d0  34 2e 31 2e 32 39 2d 4c 45 2d 6a 64 6b 31 34 3c   4.1.29-LE-jdk14<
02e0  2f 68 33 3e 3c 2f 62 6f 64 79 3e 3c 2f 68 74 6d   /h3></body></htm
02f0  6c 3e 0d 0a                                       l>..

Frame 20 (59 bytes on wire, 59 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.102922000
    Time delta from previous packet: 0.000031000 seconds
    Time since reference or first frame: 45.523918000 seconds
    Frame Number: 20
    Packet Length: 59 bytes
    Capture Length: 59 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 45
    Identification: 0x5472 (21618)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4fb1)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 34094 (34094), Seq: 957, Ack: 604, Len: 5
    Source port: 8080 (8080)
    Destination port: 34094 (34094)
    Sequence number: 957
    Next sequence number: 962
    Acknowledgement number: 604
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16917
    Checksum: 0x56c7 (incorrect, should be 0xe04a)
Hypertext Transfer Protocol
    Data (5 bytes)

0000  30 0d 0a 0d 0a                                    0....

Frame 21 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.103306000
    Time delta from previous packet: 0.000384000 seconds
    Time since reference or first frame: 45.524302000 seconds
    Frame Number: 21
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe1e8 (57832)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x0240 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 604, Ack: 957, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 604
    Acknowledgement number: 957
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x4c63 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 19
        The RTT to ACK the segment was: 0.000415000 seconds

Frame 22 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.103316000
    Time delta from previous packet: 0.000010000 seconds
    Time since reference or first frame: 45.524312000 seconds
    Frame Number: 22
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe1e9 (57833)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x023f (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 604, Ack: 962, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 604
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x4c5e (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 20
        The RTT to ACK the segment was: 0.000394000 seconds

Frame 23 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.590658000
    Time delta from previous packet: 0.487342000 seconds
    Time since reference or first frame: 46.011654000 seconds
    Frame Number: 23
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe1ea (57834)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x023e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 604, Ack: 962, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 604
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6692
    Checksum: 0x4c5d (correct)

Frame 24 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.590679000
    Time delta from previous packet: 0.000021000 seconds
    Time since reference or first frame: 46.011675000 seconds
    Frame Number: 24
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x5479 (21625)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4faf)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 34094 (34094), Seq: 962, Ack: 605, Len: 0
    Source port: 8080 (8080)
    Destination port: 34094 (34094)
    Sequence number: 962
    Acknowledgement number: 605
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16917
    Checksum: 0x56c2 (incorrect, should be 0x246c)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 23
        The RTT to ACK the segment was: 0.000021000 seconds

Frame 25 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.590842000
    Time delta from previous packet: 0.000163000 seconds
    Time since reference or first frame: 46.011838000 seconds
    Frame Number: 25
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x547a (21626)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x4fae)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 34094 (34094), Seq: 962, Ack: 605, Len: 0
    Source port: 8080 (8080)
    Destination port: 34094 (34094)
    Sequence number: 962
    Acknowledgement number: 605
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16917
    Checksum: 0x56c2 (incorrect, should be 0x246b)

Frame 26 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 13:45:18.591139000
    Time delta from previous packet: 0.000297000 seconds
    Time since reference or first frame: 46.012135000 seconds
    Frame Number: 26
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb481 (46209)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2fa7 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 34094 (34094), Dst Port: 8080 (8080), Seq: 605, Ack: 963, Len: 0
    Source port: 34094 (34094)
    Destination port: 8080 (8080)
    Sequence number: 605
    Acknowledgement number: 963
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x4c5c (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 25
        The RTT to ACK the segment was: 0.000297000 seconds
