Frame 1 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.744916000
    Time delta from previous packet: 0.000000000 seconds
    Time since reference or first frame: 0.000000000 seconds
    Frame Number: 1
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x20 (DSCP 0x08: Class Selector 1; ECN: 0x00)
        0010 00.. = Differentiated Services Codepoint: Class Selector 1 (0x08)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x079e (1950)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xe062 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 0, Ack: 0, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x0a38 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

Frame 2 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.744951000
    Time delta from previous packet: 0.000035000 seconds
    Time since reference or first frame: 0.000035000 seconds
    Frame Number: 2
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0xc1ea (49642)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xe235)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 0, Ack: 1, Len: 0
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0xb77e (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 1
        The RTT to ACK the segment was: 0.000035000 seconds

Frame 3 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.769241000
    Time delta from previous packet: 0.024290000 seconds
    Time since reference or first frame: 0.024325000 seconds
    Frame Number: 3
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x2a14 (10772)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xba14 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x1343 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 2
        The RTT to ACK the segment was: 0.024290000 seconds

Frame 4 (1426 bytes on wire, 1426 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.797939000
    Time delta from previous packet: 0.028698000 seconds
    Time since reference or first frame: 0.053023000 seconds
    Frame Number: 4
    Packet Length: 1426 bytes
    Capture Length: 1426 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 1412
    Identification: 0x2a15 (10773)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xb4b7 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 1, Ack: 1, Len: 1372
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 1
    Next sequence number: 1373
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xd09b (correct)
Hypertext Transfer Protocol
    POST /servlet/InstallNotify HTTP/1.1\r\n
        Request Method: POST
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Host: 195.235.160.80:8080\r\n
    Accept: text/html, application/xml, application/xhtml+xml, application/vnd.wap.xhtml+xml, multipart/mixed, application/vnd.wap.multipart.mixed, text/wml, text/vnd.wap.wml, image/png, image/jpeg, image/gif, image/x-xbitmap ,application/vnd.

Frame 5 (1426 bytes on wire, 1426 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.797956000
    Time delta from previous packet: 0.000017000 seconds
    Time since reference or first frame: 0.053040000 seconds
    Frame Number: 5
    Packet Length: 1426 bytes
    Capture Length: 1426 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 1412
    Identification: 0x2a16 (10774)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xb4b6 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 1373, Ack: 1, Len: 1372
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 1373
    Next sequence number: 2745
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xda95 (correct)
Hypertext Transfer Protocol
    Data (1372 bytes)

0000  2d 6d 69 64 69 2c 61 70 70 6c 69 63 61 74 69 6f   -midi,applicatio
0010  6e 2f 76 6e 64 2e 6f 6d 61 2e 64 72 6d 2e 64 63   n/vnd.oma.drm.dc
0020  66 61 2c 61 70 70 6c 69 63 61 74 69 6f 6e 2f 76   fa,application/v
0030  6e 64 2e 6f 6d 61 2e 64 72 6d 2e 64 6d 61 2c 61   nd.oma.drm.dma,a
0040  70 70 6c 69 63 61 74 69 6f 6e 2f 76 6e 64 2e 6f   pplication/vnd.o
0050  6d 61 2e 64 72 6d 2e 6f 64 66 61 2c 61 75 64 69   ma.drm.odfa,audi
0060  6f 2f 6d 70 33 2c 61 75 64 69 6f 2f 6d 70 65 67   o/mp3,audio/mpeg
0070  2c 61 75 64 69 6f 2f 6d 70 65 67 33 2c 61 75 64   ,audio/mpeg3,aud
0080  69 6f 2f 6d 70 67 2c 61 75 64 69 6f 2f 78 2d 6d   io/mpg,audio/x-m
0090  70 33 2c 61 75 64 69 6f 2f 78 2d 6d 70 65 67 2c   p3,audio/x-mpeg,
00a0  61 75 64 69 6f 2f 78 2d 6d 70 65 67 33 2c 61 75   audio/x-mpeg3,au
00b0  64 69 6f 2f 78 2d 6d 70 67 2c 61 75 64 69 6f 2f   dio/x-mpg,audio/
00c0  62 61 73 69 63 2c 61 75 64 69 6f 2f 61 75 2c 61   basic,audio/au,a
00d0  75 64 69 6f 2f 78 2d 6d 73 2d 77 6d 61 2c 61 70   udio/x-ms-wma,ap
00e0  70 6c 69 63 61 74 69 6f 6e 2f 78 2d 68 33 67 2d   plication/x-h3g-
00f0  64 72 6d 2d 6d 6d 61 2c 61 75 64 69 6f 2f 6d 70   drm-mma,audio/mp
0100  34 2c 61 75 64 69 6f 2f 33 67 70 70 2c 61 75 64   4,audio/3gpp,aud
0110  69 6f 2f 76 6e 64 2e 72 6e 2d 72 65 61 6c 61 75   io/vnd.rn-realau
0120  64 69 6f 2c 61 75 64 69 6f 2f 78 2d 70 6e 2d 72   dio,audio/x-pn-r
0130  65 61 6c 61 75 64 69 6f 2c 61 75 64 69 6f 2f 6d   ealaudio,audio/m
0140  34 61 2c 61 75 64 69 6f 2f 78 2d 6d 34 61 2c 61   4a,audio/x-m4a,a
0150  75 64 69 6f 2f 61 6d 72 2c 61 75 64 69 6f 2f 61   udio/amr,audio/a
0160  6d 72 2d 77 62 2c 74 65 78 74 2f 76 6e 64 2e 73   mr-wb,text/vnd.s
0170  75 6e 2e 6a 32 6d 65 2e 61 70 70 2d 64 65 73 63   un.j2me.app-desc
0180  72 69 70 74 6f 72 2c 61 70 70 6c 69 63 61 74 69   riptor,applicati
0190  6f 6e 2f 6a 61 76 61 2d 61 72 63 68 69 76 65 2c   on/java-archive,
01a0  61 70 70 6c 69 63 61 74 69 6f 6e 2f 76 6e 64 2e   application/vnd.
01b0  6f 6d 61 2e 64 72 6d 2e 64 6d 6a 2c 61 70 70 6c   oma.drm.dmj,appl
01c0  69 63 61 74 69 6f 6e 2f 76 6e 64 2e 6f 6d 61 2e   ication/vnd.oma.
01d0  64 72 6d 2e 64 63 66 6a 2c 74 65 78 74 2f 70 6c   drm.dcfj,text/pl
01e0  61 69 6e 2c 61 70 70 6c 69 63 61 74 69 6f 6e 2f   ain,application/
01f0  6f 63 74 65 74 2d 73 74 72 65 61 6d 20 2c 61 70   octet-stream ,ap
0200  70 6c 69 63 61 74 69 6f 6e 2f 76 6e 64 2e 77 61   plication/vnd.wa
0210  70 2e 6d 6d 73 2d 6d 65 73 73 61 67 65 20 2c 2a   p.mms-message ,*
0220  2f 2a 2c 2a 2f 2a 0d 0a 41 63 63 65 70 74 2d 61   /*,*/*..Accept-a
0230  70 70 6c 69 63 61 74 69 6f 6e 3a 20 78 2d 77 61   pplication: x-wa
0240  70 2d 61 70 70 6c 69 63 61 74 69 6f 6e 3a 77 6d   p-application:wm
0250  6c 2e 75 61 2c 78 2d 77 61 70 2d 61 70 70 6c 69   l.ua,x-wap-appli
0260  63 61 74 69 6f 6e 3a 6d 6d 73 2e 75 61 0d 0a 41   cation:mms.ua..A
0270  63 63 65 70 74 2d 43 68 61 72 73 65 74 3a 20 69   ccept-Charset: i
0280  73 6f 2d 38 38 35 39 2d 31 2c 20 75 74 66 2d 38   so-8859-1, utf-8
0290  2c 20 75 74 66 2d 31 36 2c 20 2a 3b 71 3d 30 2e   , utf-16, *;q=0.
02a0  31 2c 2a 0d 0a 41 63 63 65 70 74 2d 45 6e 63 6f   1,*..Accept-Enco
02b0  64 69 6e 67 3a 20 67 7a 69 70 2c 20 64 65 66 6c   ding: gzip, defl
02c0  61 74 65 0d 0a 43 6f 6e 74 65 6e 74 2d 4c 65 6e   ate..Content-Len
02d0  67 74 68 3a 20 31 31 0d 0a 55 73 65 72 2d 41 67   gth: 11..User-Ag
02e0  65 6e 74 3a 20 4d 4f 54 2d 52 41 5a 52 56 33 78   ent: MOT-RAZRV3x
02f0  78 2f 39 39 2e 30 34 2e 31 30 52 20 42 45 52 32   x/99.04.10R BER2
0300  2e 32 20 4d 6f 7a 69 6c 6c 61 2f 34 2e 30 20 28   .2 Mozilla/4.0 (
0310  63 6f 6d 70 61 74 69 62 6c 65 3b 20 4d 53 49 45   compatible; MSIE
0320  20 36 2e 30 3b 20 31 32 30 30 33 31 30 31 29 20    6.0; 12003101) 
0330  50 72 6f 66 69 6c 65 2f 4d 49 44 50 2d 32 2e 30   Profile/MIDP-2.0
0340  20 43 6f 6e 66 69 67 75 72 61 74 69 6f 6e 2f 43    Configuration/C
0350  4c 44 43 2d 31 2e 31 20 20 4f 70 65 72 61 20 38   LDC-1.1  Opera 8
0360  2e 30 30 20 5b 65 73 5d 20 55 50 2e 4c 69 6e 6b   .00 [es] UP.Link
0370  2f 36 2e 33 2e 31 2e 31 34 2e 30 0d 0a 58 2d 57   /6.3.1.14.0..X-W
0380  61 70 2d 50 72 6f 66 69 6c 65 3a 20 22 68 74 74   ap-Profile: "htt
0390  70 3a 2f 2f 6d 6f 74 6f 72 6f 6c 61 2e 68 61 6e   p://motorola.han
03a0  64 61 6e 67 6f 2e 63 6f 6d 2f 70 68 6f 6e 65 63   dango.com/phonec
03b0  6f 6e 66 69 67 2f 72 61 7a 72 76 33 78 78 2f 50   onfig/razrv3xx/P
03c0  72 6f 66 69 6c 65 2f 52 41 5a 52 56 33 78 78 2e   rofile/RAZRV3xx.
03d0  72 64 66 22 0d 0a 78 2d 75 70 2d 64 65 76 63 61   rdf"..x-up-devca
03e0  70 2d 73 6d 61 72 74 64 69 61 6c 69 6e 67 3a 20   p-smartdialing: 
03f0  31 0d 0a 78 2d 75 70 2d 64 65 76 63 61 70 2d 69   1..x-up-devcap-i
0400  73 63 6f 6c 6f 72 3a 20 31 0d 0a 78 2d 75 70 2d   scolor: 1..x-up-
0410  64 65 76 63 61 70 2d 73 63 72 65 65 6e 64 65 70   devcap-screendep
0420  74 68 3a 20 31 36 0d 0a 78 2d 75 70 2d 64 65 76   th: 16..x-up-dev
0430  63 61 70 2d 6e 75 6d 73 6f 66 74 6b 65 79 73 3a   cap-numsoftkeys:
0440  20 32 0d 0a 78 2d 75 70 2d 64 65 76 63 61 70 2d    2..x-up-devcap-
0450  63 68 61 72 73 65 74 3a 20 75 74 66 2d 38 2c 49   charset: utf-8,I
0460  53 4f 2d 38 38 35 39 2d 31 2c 55 53 2d 41 53 43   SO-8859-1,US-ASC
0470  49 49 2c 55 54 46 2d 31 36 2c 47 42 2d 32 33 31   II,UTF-16,GB-231
0480  32 2c 42 49 47 2d 35 0d 0a 78 2d 75 70 2d 64 65   2,BIG-5..x-up-de
0490  76 63 61 70 2d 73 63 72 65 65 6e 70 69 78 65 6c   vcap-screenpixel
04a0  73 3a 20 32 34 30 2c 33 32 30 0d 0a 78 2d 75 70   s: 240,320..x-up
04b0  2d 64 65 76 63 61 70 2d 6d 61 78 2d 70 64 75 3a   -devcap-max-pdu:
04c0  20 34 31 39 34 33 30 34 0d 0a 78 2d 75 70 2d 64    4194304..x-up-d
04d0  65 76 63 61 70 2d 61 63 63 65 70 74 2d 6c 61 6e   evcap-accept-lan
04e0  67 75 61 67 65 3a 20 65 6e 0d 0a 78 2d 75 70 2d   guage: en..x-up-
04f0  66 6f 72 77 61 72 64 65 64 2d 66 6f 72 3a 20 31   forwarded-for: 1
0500  30 2e 31 34 36 2e 34 34 2e 31 35 31 0d 0a 78 2d   0.146.44.151..x-
0510  75 70 2d 73 75 62 73 63 72 69 62 65 72 2d 63 6f   up-subscriber-co
0520  69 3a 20 63 6f 69 77 61 70 0d 0a 56 69 61 3a 20   i: coiwap..Via: 
0530  31 2e 31 20 6d 62 65 2d 70 72 6f 78 79 38 70 65   1.1 mbe-proxy8pe
0540  2e 77 61 70 2e 6f 6c 65 61 64 61 2e 63 6f 6d 3a   .wap.oleada.com:
0550  38 30 38 30 0d 0a 0d 0a 39 30 30 20               8080....900 

Frame 6 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.797969000
    Time delta from previous packet: 0.000013000 seconds
    Time since reference or first frame: 0.053053000 seconds
    Frame Number: 6
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xc1eb (49643)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xe23c)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 1, Ack: 2745, Len: 0
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 1
    Acknowledgement number: 2745
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x56c2 (incorrect, should be 0xd98a)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 5
        The RTT to ACK the segment was: 0.000013000 seconds

Frame 7 (61 bytes on wire, 61 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.798172000
    Time delta from previous packet: 0.000203000 seconds
    Time since reference or first frame: 0.053256000 seconds
    Frame Number: 7
    Packet Length: 61 bytes
    Capture Length: 61 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 47
    Identification: 0x2a17 (10775)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xba0a (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 2745, Ack: 1, Len: 7
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 2745
    Next sequence number: 2752
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x792f (correct)
Hypertext Transfer Protocol
    Data (7 bytes)

0000  53 75 63 63 65 73 73                              Success

Frame 8 (1010 bytes on wire, 1010 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.802135000
    Time delta from previous packet: 0.003963000 seconds
    Time since reference or first frame: 0.057219000 seconds
    Frame Number: 8
    Packet Length: 1010 bytes
    Capture Length: 1010 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 996
    Identification: 0xc1ec (49644)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xde7f)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 1, Ack: 2752, Len: 956
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 1
    Next sequence number: 957
    Acknowledgement number: 2752
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 17513
    Checksum: 0x5a7e (incorrect, should be 0xb704)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 7
        The RTT to ACK the segment was: 0.003963000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 404 /servlet/InstallNotify\r\n
        Response Code: 404
    Content-Type: text/html;charset=ISO-8859-1\r\n
    Content-Language: es-ES\r\n
    Transfer-Encoding: chunked\r\n
    Date: Wed, 20 Dec 2006 13:21:22 GMT\r\n
    Server: Apache-Coyote/1.1\r\n
    \r\n
    Data (756 bytes)

0000  32 65 64 0d 0a 3c 68 74 6d 6c 3e 3c 68 65 61 64   2ed..<html><head
0010  3e 3c 74 69 74 6c 65 3e 41 70 61 63 68 65 20 54   ><title>Apache T
0020  6f 6d 63 61 74 2f 34 2e 31 2e 32 39 2d 4c 45 2d   omcat/4.1.29-LE-
0030  6a 64 6b 31 34 20 2d 20 45 72 72 6f 72 20 72 65   jdk14 - Error re
0040  70 6f 72 74 3c 2f 74 69 74 6c 65 3e 3c 53 54 59   port</title><STY
0050  4c 45 3e 3c 21 2d 2d 48 31 7b 66 6f 6e 74 2d 66   LE><!--H1{font-f
0060  61 6d 69 6c 79 20 3a 20 73 61 6e 73 2d 73 65 72   amily : sans-ser
0070  69 66 2c 41 72 69 61 6c 2c 54 61 68 6f 6d 61 3b   if,Arial,Tahoma;
0080  63 6f 6c 6f 72 20 3a 20 77 68 69 74 65 3b 62 61   color : white;ba
0090  63 6b 67 72 6f 75 6e 64 2d 63 6f 6c 6f 72 20 3a   ckground-color :
00a0  20 23 30 30 38 36 62 32 3b 7d 20 48 33 7b 66 6f    #0086b2;} H3{fo
00b0  6e 74 2d 66 61 6d 69 6c 79 20 3a 20 73 61 6e 73   nt-family : sans
00c0  2d 73 65 72 69 66 2c 41 72 69 61 6c 2c 54 61 68   -serif,Arial,Tah
00d0  6f 6d 61 3b 63 6f 6c 6f 72 20 3a 20 77 68 69 74   oma;color : whit
00e0  65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f 6c   e;background-col
00f0  6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20 42   or : #0086b2;} B
0100  4f 44 59 7b 66 6f 6e 74 2d 66 61 6d 69 6c 79 20   ODY{font-family 
0110  3a 20 73 61 6e 73 2d 73 65 72 69 66 2c 41 72 69   : sans-serif,Ari
0120  61 6c 2c 54 61 68 6f 6d 61 3b 63 6f 6c 6f 72 20   al,Tahoma;color 
0130  3a 20 62 6c 61 63 6b 3b 62 61 63 6b 67 72 6f 75   : black;backgrou
0140  6e 64 2d 63 6f 6c 6f 72 20 3a 20 77 68 69 74 65   nd-color : white
0150  3b 7d 20 42 7b 63 6f 6c 6f 72 20 3a 20 77 68 69   ;} B{color : whi
0160  74 65 3b 62 61 63 6b 67 72 6f 75 6e 64 2d 63 6f   te;background-co
0170  6c 6f 72 20 3a 20 23 30 30 38 36 62 32 3b 7d 20   lor : #0086b2;} 
0180  48 52 7b 63 6f 6c 6f 72 20 3a 20 23 30 30 38 36   HR{color : #0086
0190  62 32 3b 7d 20 2d 2d 3e 3c 2f 53 54 59 4c 45 3e   b2;} --></STYLE>
01a0  20 3c 2f 68 65 61 64 3e 3c 62 6f 64 79 3e 3c 68    </head><body><h
01b0  31 3e 48 54 54 50 20 53 74 61 74 75 73 20 34 30   1>HTTP Status 40
01c0  34 20 2d 20 2f 73 65 72 76 6c 65 74 2f 49 6e 73   4 - /servlet/Ins
01d0  74 61 6c 6c 4e 6f 74 69 66 79 3c 2f 68 31 3e 3c   tallNotify</h1><
01e0  48 52 20 73 69 7a 65 3d 22 31 22 20 6e 6f 73 68   HR size="1" nosh
01f0  61 64 65 3e 3c 70 3e 3c 62 3e 74 79 70 65 3c 2f   ade><p><b>type</
0200  62 3e 20 53 74 61 74 75 73 20 72 65 70 6f 72 74   b> Status report
0210  3c 2f 70 3e 3c 70 3e 3c 62 3e 6d 65 73 73 61 67   </p><p><b>messag
0220  65 3c 2f 62 3e 20 3c 75 3e 2f 73 65 72 76 6c 65   e</b> <u>/servle
0230  74 2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 3c   t/InstallNotify<
0240  2f 75 3e 3c 2f 70 3e 3c 70 3e 3c 62 3e 64 65 73   /u></p><p><b>des
0250  63 72 69 70 74 69 6f 6e 3c 2f 62 3e 20 3c 75 3e   cription</b> <u>
0260  54 68 65 20 72 65 71 75 65 73 74 65 64 20 72 65   The requested re
0270  73 6f 75 72 63 65 20 28 2f 73 65 72 76 6c 65 74   source (/servlet
0280  2f 49 6e 73 74 61 6c 6c 4e 6f 74 69 66 79 29 20   /InstallNotify) 
0290  69 73 20 6e 6f 74 20 61 76 61 69 6c 61 62 6c 65   is not available
02a0  2e 3c 2f 75 3e 3c 2f 70 3e 3c 48 52 20 73 69 7a   .</u></p><HR siz
02b0  65 3d 22 31 22 20 6e 6f 73 68 61 64 65 3e 3c 68   e="1" noshade><h
02c0  33 3e 41 70 61 63 68 65 20 54 6f 6d 63 61 74 2f   3>Apache Tomcat/
02d0  34 2e 31 2e 32 39 2d 4c 45 2d 6a 64 6b 31 34 3c   4.1.29-LE-jdk14<
02e0  2f 68 33 3e 3c 2f 62 6f 64 79 3e 3c 2f 68 74 6d   /h3></body></htm
02f0  6c 3e 0d 0a                                       l>..

Frame 9 (59 bytes on wire, 59 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.802167000
    Time delta from previous packet: 0.000032000 seconds
    Time since reference or first frame: 0.057251000 seconds
    Frame Number: 9
    Packet Length: 59 bytes
    Capture Length: 59 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 45
    Identification: 0xc1ed (49645)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xe235)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 957, Ack: 2752, Len: 5
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 957
    Next sequence number: 962
    Acknowledgement number: 2752
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 17513
    Checksum: 0x56c7 (incorrect, should be 0x91a7)
Hypertext Transfer Protocol
    Data (5 bytes)

0000  30 0d 0a 0d 0a                                    0....

Frame 10 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.802796000
    Time delta from previous packet: 0.000629000 seconds
    Time since reference or first frame: 0.057880000 seconds
    Frame Number: 10
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x2a18 (10776)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xba10 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 2752, Ack: 957, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 2752
    Acknowledgement number: 957
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x0014 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 8
        The RTT to ACK the segment was: 0.000661000 seconds

Frame 11 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:22.802806000
    Time delta from previous packet: 0.000010000 seconds
    Time since reference or first frame: 0.057890000 seconds
    Frame Number: 11
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x2a19 (10777)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xba0f (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 2752, Ack: 962, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 2752
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x000f (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 9
        The RTT to ACK the segment was: 0.000639000 seconds

Frame 12 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:23.064231000
    Time delta from previous packet: 0.261425000 seconds
    Time since reference or first frame: 0.319315000 seconds
    Frame Number: 12
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x2a1a (10778)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xba0e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 2752, Ack: 962, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 2752
    Acknowledgement number: 962
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6692
    Checksum: 0x000e (correct)

Frame 13 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:23.064254000
    Time delta from previous packet: 0.000023000 seconds
    Time since reference or first frame: 0.319338000 seconds
    Frame Number: 13
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xc1f4 (49652)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xe233)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 962, Ack: 2753, Len: 0
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 962
    Acknowledgement number: 2753
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 17513
    Checksum: 0x56c2 (incorrect, should be 0xd5c8)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 12
        The RTT to ACK the segment was: 0.000023000 seconds

Frame 14 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:23.064424000
    Time delta from previous packet: 0.000170000 seconds
    Time since reference or first frame: 0.319508000 seconds
    Frame Number: 14
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xc1f5 (49653)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0xe232)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: 8080 (8080), Dst Port: 40427 (40427), Seq: 962, Ack: 2753, Len: 0
    Source port: 8080 (8080)
    Destination port: 40427 (40427)
    Sequence number: 962
    Acknowledgement number: 2753
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 17513
    Checksum: 0x56c2 (incorrect, should be 0xd5c7)

Frame 15 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Dec 20, 2006 14:21:23.064707000
    Time delta from previous packet: 0.000283000 seconds
    Time since reference or first frame: 0.319791000 seconds
    Frame Number: 15
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xb5e9 (46569)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x2e3f (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 40427 (40427), Dst Port: 8080 (8080), Seq: 2753, Ack: 963, Len: 0
    Source port: 40427 (40427)
    Destination port: 8080 (8080)
    Sequence number: 2753
    Acknowledgement number: 963
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6692
    Checksum: 0x000d (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 14
        The RTT to ACK the segment was: 0.000283000 seconds
