Frame 1 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.121349000
    Time delta from previous packet: 0.000000000 seconds
    Time since reference or first frame: 0.000000000 seconds
    Frame Number: 1
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0xefe5 (61413)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xf7da (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x40b7 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 ef e5 40 00 3c 06 f7 da c3 37 2f 34 c3 eb   .0..@.<....7/4..
0020  a0 50 b9 88 00 50 4f 48 81 ab 00 00 00 00 70 02   .P...POH......p.
0030  60 f4 40 b7 00 00 02 04 05 b4 01 01 04 02         `.@...........

Frame 2 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.121381000
    Time delta from previous packet: 0.000032000 seconds
    Time since reference or first frame: 0.000032000 seconds
    Frame Number: 2
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7566 (30054)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eba)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47496 (47496), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 47496 (47496)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x27ee (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 1
        The RTT to ACK the segment was: 0.000032000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 66 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0uf@........P.7
0020  2f 34 00 50 b9 88 bb fa 79 41 4f 48 81 ac 70 12   /4.P....yAOH..p.
0030  44 70 27 ee 00 00 02 04 05 b4 01 01 04 02         Dp'...........

Frame 3 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.170482000
    Time delta from previous packet: 0.049101000 seconds
    Time since reference or first frame: 0.049133000 seconds
    Frame Number: 3
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x8933 (35123)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x5af5 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x83b2 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 2
        The RTT to ACK the segment was: 0.049101000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 89 33 40 00 40 06 5a f5 c3 37 2f 34 c3 eb   .(.3@.@.Z..7/4..
0020  a0 50 b9 88 00 50 4f 48 81 ac bb fa 79 42 50 10   .P...POH....yBP.
0030  15 70 83 b2 00 00 00 00 00 00 00 00               .p..........

Frame 4 (750 bytes on wire, 750 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.172418000
    Time delta from previous packet: 0.001936000 seconds
    Time since reference or first frame: 0.051069000 seconds
    Frame Number: 4
    Packet Length: 750 bytes
    Capture Length: 750 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 736
    Identification: 0x8934 (35124)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x583c (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 1, Ack: 1, Len: 696
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 697
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xfb5d (correct)
Hypertext Transfer Protocol
    GET /java/index.wml HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/index.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  02 e0 89 34 40 00 40 06 58 3c c3 37 2f 34 c3 eb   ...4@.@.X<.7/4..
0020  a0 50 b9 88 00 50 4f 48 81 ac bb fa 79 42 50 18   .P...POH....yBP.
0030  15 70 fb 5d 00 00 47 45 54 20 2f 6a 61 76 61 2f   .p.]..GET /java/
0040  69 6e 64 65 78 2e 77 6d 6c 20 48 54 54 50 2f 31   index.wml HTTP/1
0050  2e 31 0d 0a 54 4d 5f 75 73 65 72 2d 69 64 3a 20   .1..TM_user-id: 
0060  30 33 34 36 30 32 37 33 38 34 33 31 35 34 36 31   0346027384315461
0070  33 30 37 0d 0a 78 2d 75 70 2d 73 75 62 6e 6f 3a   307..x-up-subno:
0080  20 30 33 34 36 30 32 37 33 38 34 33 31 35 34 36    034602738431546
0090  31 33 30 37 0d 0a 48 6f 73 74 3a 20 31 39 35 2e   1307..Host: 195.
00a0  32 33 35 2e 31 36 30 2e 38 30 0d 0a 41 63 63 65   235.160.80..Acce
00b0  70 74 3a 20 6d 75 6c 74 69 70 61 72 74 2f 6d 69   pt: multipart/mi
00c0  78 65 64 2c 20 61 70 70 6c 69 63 61 74 69 6f 6e   xed, application
00d0  2f 76 6e 64 2e 77 61 70 2e 6d 75 6c 74 69 70 61   /vnd.wap.multipa
00e0  72 74 2e 6d 69 78 65 64 2c 20 61 70 70 6c 69 63   rt.mixed, applic
00f0  61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70 2e 78 68   ation/vnd.wap.xh
0100  74 6d 6c 2b 78 6d 6c 2c 20 61 70 70 6c 69 63 61   tml+xml, applica
0110  74 69 6f 6e 2f 78 68 74 6d 6c 2b 78 6d 6c 2c 20   tion/xhtml+xml, 
0120  74 65 78 74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c   text/vnd.wap.wml
0130  2c 20 2a 2f 2a 2c 2a 2f 2a 0d 0a 41 63 63 65 70   , */*,*/*..Accep
0140  74 2d 43 68 61 72 73 65 74 3a 20 75 74 66 2d 38   t-Charset: utf-8
0150  2c 20 75 74 66 2d 31 36 2c 20 69 73 6f 2d 38 38   , utf-16, iso-88
0160  35 39 2d 31 2c 20 69 73 6f 2d 31 30 36 34 36 2d   59-1, iso-10646-
0170  75 63 73 2d 32 2c 20 53 68 69 66 74 5f 4a 49 53   ucs-2, Shift_JIS
0180  2c 20 42 69 67 35 2c 2a 0d 0a 41 63 63 65 70 74   , Big5,*..Accept
0190  2d 45 6e 63 6f 64 69 6e 67 3a 20 67 7a 69 70 2c   -Encoding: gzip,
01a0  20 64 65 66 6c 61 74 65 0d 0a 41 63 63 65 70 74    deflate..Accept
01b0  2d 4c 61 6e 67 75 61 67 65 3a 20 65 73 0d 0a 52   -Language: es..R
01c0  65 66 65 72 65 72 3a 20 68 74 74 70 3a 2f 2f 31   eferer: http://1
01d0  39 35 2e 32 33 35 2e 31 36 30 2e 38 30 2f 69 6e   95.235.160.80/in
01e0  64 65 78 2e 77 6d 6c 0d 0a 55 73 65 72 2d 41 67   dex.wml..User-Ag
01f0  65 6e 74 3a 20 53 6f 6e 79 45 72 69 63 73 73 6f   ent: SonyEricsso
0200  6e 5a 35 33 30 69 2f 52 36 41 43 20 42 72 6f 77   nZ530i/R6AC Brow
0210  73 65 72 2f 4e 65 74 46 72 6f 6e 74 2f 33 2e 33   ser/NetFront/3.3
0220  20 50 72 6f 66 69 6c 65 2f 4d 49 44 50 2d 32 2e    Profile/MIDP-2.
0230  30 20 43 6f 6e 66 69 67 75 72 61 74 69 6f 6e 2f   0 Configuration/
0240  43 4c 44 43 2d 31 2e 31 20 55 50 2e 4c 69 6e 6b   CLDC-1.1 UP.Link
0250  2f 36 2e 32 2e 33 2e 31 35 2e 30 0d 0a 78 2d 77   /6.2.3.15.0..x-w
0260  61 70 2d 70 72 6f 66 69 6c 65 3a 20 22 68 74 74   ap-profile: "htt
0270  70 3a 2f 2f 77 61 70 2e 73 6f 6e 79 65 72 69 63   p://wap.sonyeric
0280  73 73 6f 6e 2e 63 6f 6d 2f 55 41 70 72 6f 66 2f   sson.com/UAprof/
0290  5a 35 33 30 69 52 32 30 31 2e 78 6d 6c 22 0d 0a   Z530iR201.xml"..
02a0  78 2d 75 70 2d 66 6f 72 77 61 72 64 65 64 2d 66   x-up-forwarded-f
02b0  6f 72 3a 20 31 30 2e 31 34 36 2e 36 33 2e 30 0d   or: 10.146.63.0.
02c0  0a 56 69 61 3a 20 31 2e 31 20 6d 62 65 2d 70 72   .Via: 1.1 mbe-pr
02d0  6f 78 79 32 70 65 2e 77 61 70 2e 6f 6c 65 61 64   oxy2pe.wap.olead
02e0  61 2e 63 6f 6d 3a 38 30 38 30 0d 0a 0d 0a         a.com:8080....

Frame 5 (730 bytes on wire, 730 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.173170000
    Time delta from previous packet: 0.000752000 seconds
    Time since reference or first frame: 0.051821000 seconds
    Frame Number: 5
    Packet Length: 730 bytes
    Capture Length: 730 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 716
    Identification: 0x7567 (30055)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2c1d)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47496 (47496), Seq: 1, Ack: 697, Len: 676
    Source port: http (80)
    Destination port: 47496 (47496)
    Sequence number: 1
    Next sequence number: 677
    Acknowledgement number: 697
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16824
    Checksum: 0x5966 (incorrect, should be 0x6c0d)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 4
        The RTT to ACK the segment was: 0.000752000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:14 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Tue, 18 Apr 2006 09:05:40 GMT\r\n
    ETag: "0-1bc-4444abe4"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 444\r\n
    Content-Type: text/vnd.wap.wml\r\n
    \r\n
    Data (444 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  02 cc 75 67 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..ug@........P.7
0020  2f 34 00 50 b9 88 bb fa 79 42 4f 48 84 64 50 18   /4.P....yBOH.dP.
0030  41 b8 59 66 00 00 48 54 54 50 2f 31 2e 31 20 32   A.Yf..HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 31 34 20 47 4d 54 0d 0a 53 65 72 76   :42:14 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 54 75 65 2c 20 31   Modified: Tue, 1
00a0  38 20 41 70 72 20 32 30 30 36 20 30 39 3a 30 35   8 Apr 2006 09:05
00b0  3a 34 30 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :40 GMT..ETag: "
00c0  30 2d 31 62 63 2d 34 34 34 34 61 62 65 34 22 0d   0-1bc-4444abe4".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 34 34 34 0d 0a 43 6f 6e 74   ength: 444..Cont
0100  65 6e 74 2d 54 79 70 65 3a 20 74 65 78 74 2f 76   ent-Type: text/v
0110  6e 64 2e 77 61 70 2e 77 6d 6c 0d 0a 0d 0a 3c 3f   nd.wap.wml....<?
0120  78 6d 6c 20 76 65 72 73 69 6f 6e 3d 22 31 2e 30   xml version="1.0
0130  22 3f 3e 20 0d 0a 3c 21 44 4f 43 54 59 50 45 20   "?> ..<!DOCTYPE 
0140  77 6d 6c 20 50 55 42 4c 49 43 20 22 2d 2f 2f 57   wml PUBLIC "-//W
0150  41 50 46 4f 52 55 4d 2f 2f 44 54 44 20 57 4d 4c   APFORUM//DTD WML
0160  20 31 2e 31 2f 2f 45 4e 22 20 22 68 74 74 70 3a    1.1//EN" "http:
0170  2f 2f 77 77 77 2e 77 61 70 66 6f 72 75 6d 2e 6f   //www.wapforum.o
0180  72 67 2f 44 54 44 2f 77 6d 6c 5f 31 2e 31 2e 78   rg/DTD/wml_1.1.x
0190  6d 6c 22 3e 20 0d 0a 0d 0a 3c 77 6d 6c 3e 0d 0a   ml"> ....<wml>..
01a0  0d 0a 3c 68 65 61 64 3e 20 0d 0a 3c 6d 65 74 61   ..<head> ..<meta
01b0  20 68 74 74 70 2d 65 71 75 69 76 3d 22 43 6f 6e    http-equiv="Con
01c0  74 65 6e 74 2d 54 79 70 65 22 20 63 6f 6e 74 65   tent-Type" conte
01d0  6e 74 3d 22 74 65 78 74 2f 76 6e 64 2e 77 61 70   nt="text/vnd.wap
01e0  2e 77 6d 6c 3b 20 63 68 61 72 73 65 74 3d 69 73   .wml; charset=is
01f0  6f 2d 38 38 35 39 2d 31 22 2f 3e 0d 0a 3c 2f 68   o-8859-1"/>..</h
0200  65 61 64 3e 0d 0a 0d 0a 3c 63 61 72 64 20 74 69   ead>....<card ti
0210  74 6c 65 3d 22 4a 61 76 61 20 69 6e 64 65 78 22   tle="Java index"
0220  3e 0d 0a 20 3c 70 3e 0d 0a 20 20 4a 61 76 61 20   >.. <p>..  Java 
0230  6d 65 6e 75 3a 3c 62 72 2f 3e 0d 0a 20 20 3c 61   menu:<br/>..  <a
0240  20 68 72 65 66 3d 22 6d 69 64 70 2e 77 6d 6c 22    href="midp.wml"
0250  3e 26 67 74 3b 4d 49 44 50 3c 2f 61 3e 3c 62 72   >&gt;MIDP</a><br
0260  2f 3e 0d 0a 20 20 3c 61 20 68 72 65 66 3d 22 2e   />..  <a href=".
0270  2e 2f 69 6d 6f 64 65 2f 64 6f 6a 61 2e 68 74 6d   ./imode/doja.htm
0280  6c 22 3e 26 67 74 3b 44 6f 4a 61 3c 2f 61 3e 3c   l">&gt;DoJa</a><
0290  62 72 2f 3e 0d 0a 20 20 3c 61 20 68 72 65 66 3d   br/>..  <a href=
02a0  22 72 2e 77 6d 6c 22 3e 26 67 74 3b 6a 61 76 61   "r.wml">&gt;java
02b0  20 6d 69 73 63 3c 2f 61 3e 3c 62 72 2f 3e 20 20    misc</a><br/>  
02c0  0d 0a 20 3c 2f 70 3e 0d 0a 3c 2f 63 61 72 64 3e   .. </p>..</card>
02d0  0d 0a 0d 0a 3c 2f 77 6d 6c 3e                     ....</wml>

Frame 6 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:14.173874000
    Time delta from previous packet: 0.000704000 seconds
    Time since reference or first frame: 0.052525000 seconds
    Frame Number: 6
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x8935 (35125)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x5af3 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 697, Ack: 677, Len: 0
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 697
    Acknowledgement number: 677
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6760
    Checksum: 0x795e (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 5
        The RTT to ACK the segment was: 0.000704000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 89 35 40 00 40 06 5a f3 c3 37 2f 34 c3 eb   .(.5@.@.Z..7/4..
0020  a0 50 b9 88 00 50 4f 48 84 64 bb fa 7b e6 50 10   .P...POH.d..{.P.
0030  1a 68 79 5e 00 00 00 00 00 00 00 00               .hy^........

Frame 7 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:17.165816000
    Time delta from previous packet: 2.991942000 seconds
    Time since reference or first frame: 3.044467000 seconds
    Frame Number: 7
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x8936 (35126)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x5af2 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 697, Ack: 677, Len: 0
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 697
    Acknowledgement number: 677
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6760
    Checksum: 0x795d (correct)

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 89 36 40 00 40 06 5a f2 c3 37 2f 34 c3 eb   .(.6@.@.Z..7/4..
0020  a0 50 b9 88 00 50 4f 48 84 64 bb fa 7b e6 50 11   .P...POH.d..{.P.
0030  1a 68 79 5d 00 00 00 00 00 00 00 00               .hy]........

Frame 8 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:17.165853000
    Time delta from previous packet: 0.000037000 seconds
    Time since reference or first frame: 3.044504000 seconds
    Frame Number: 8
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x756b (30059)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2ebd)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47496 (47496), Seq: 677, Ack: 698, Len: 0
    Source port: http (80)
    Destination port: 47496 (47496)
    Sequence number: 677
    Acknowledgement number: 698
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16824
    Checksum: 0x56c2 (incorrect, should be 0x520d)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 7
        The RTT to ACK the segment was: 0.000037000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 6b 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(uk@........P.7
0020  2f 34 00 50 b9 88 bb fa 7b e6 4f 48 84 65 50 10   /4.P....{.OH.eP.
0030  41 b8 56 c2 00 00                                 A.V...

Frame 9 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:17.165920000
    Time delta from previous packet: 0.000067000 seconds
    Time since reference or first frame: 3.044571000 seconds
    Frame Number: 9
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x756c (30060)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2ebc)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47496 (47496), Seq: 677, Ack: 698, Len: 0
    Source port: http (80)
    Destination port: 47496 (47496)
    Sequence number: 677
    Acknowledgement number: 698
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16824
    Checksum: 0x56c2 (incorrect, should be 0x520c)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 6c 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(ul@........P.7
0020  2f 34 00 50 b9 88 bb fa 7b e6 4f 48 84 65 50 11   /4.P....{.OH.eP.
0030  41 b8 56 c2 00 00                                 A.V...

Frame 10 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:17.166290000
    Time delta from previous packet: 0.000370000 seconds
    Time since reference or first frame: 3.044941000 seconds
    Frame Number: 10
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe719 (59161)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xfd0e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47496 (47496), Dst Port: http (80), Seq: 698, Ack: 678, Len: 0
    Source port: 47496 (47496)
    Destination port: http (80)
    Sequence number: 698
    Acknowledgement number: 678
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6760
    Checksum: 0x795c (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 9
        The RTT to ACK the segment was: 0.000370000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 e7 19 40 00 40 06 fd 0e c3 37 2f 34 c3 eb   .(..@.@....7/4..
0020  a0 50 b9 88 00 50 4f 48 84 65 bb fa 7b e7 50 10   .P...POH.e..{.P.
0030  1a 68 79 5c 00 00 00 00 00 00 00 00               .hy\........

Frame 11 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.576292000
    Time delta from previous packet: 1.410002000 seconds
    Time since reference or first frame: 4.454943000 seconds
    Frame Number: 11
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0xc230 (49712)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0x2590 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47671 (47671), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 47671 (47671)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x1d0c (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 c2 30 40 00 3c 06 25 90 c3 37 2f 34 c3 eb   .0.0@.<.%..7/4..
0020  a0 50 ba 37 00 50 57 85 9c 6a 00 00 00 00 70 02   .P.7.PW..j....p.
0030  60 f4 1d 0c 00 00 02 04 05 b4 01 01 04 02         `.............

Frame 12 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.576327000
    Time delta from previous packet: 0.000035000 seconds
    Time since reference or first frame: 4.454978000 seconds
    Frame Number: 12
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x756e (30062)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eb2)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47671 (47671), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 47671 (47671)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x6758 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 11
        The RTT to ACK the segment was: 0.000035000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 6e 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0un@........P.7
0020  2f 34 00 50 ba 37 90 29 41 fd 57 85 9c 6b 70 12   /4.P.7.)A.W..kp.
0030  44 70 67 58 00 00 02 04 05 b4 01 01 04 02         DpgX..........

Frame 13 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.631495000
    Time delta from previous packet: 0.055168000 seconds
    Time since reference or first frame: 4.510146000 seconds
    Frame Number: 13
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x99e8 (39400)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x4a40 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47671 (47671), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 47671 (47671)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xc31c (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 12
        The RTT to ACK the segment was: 0.055168000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 99 e8 40 00 40 06 4a 40 c3 37 2f 34 c3 eb   .(..@.@.J@.7/4..
0020  a0 50 ba 37 00 50 57 85 9c 6b 90 29 41 fe 50 10   .P.7.PW..k.)A.P.
0030  15 70 c3 1c 00 00 00 00 00 00 00 00               .p..........

Frame 14 (773 bytes on wire, 773 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.642684000
    Time delta from previous packet: 0.011189000 seconds
    Time since reference or first frame: 4.521335000 seconds
    Frame Number: 14
    Packet Length: 773 bytes
    Capture Length: 773 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 759
    Identification: 0x99e9 (39401)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x4770 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47671 (47671), Dst Port: http (80), Seq: 1, Ack: 1, Len: 719
    Source port: 47671 (47671)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 720
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x7079 (correct)
Hypertext Transfer Protocol
    GET /java/midp.wml HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Connection: close\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/java/index.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  02 f7 99 e9 40 00 40 06 47 70 c3 37 2f 34 c3 eb   ....@.@.Gp.7/4..
0020  a0 50 ba 37 00 50 57 85 9c 6b 90 29 41 fe 50 18   .P.7.PW..k.)A.P.
0030  15 70 70 79 00 00 47 45 54 20 2f 6a 61 76 61 2f   .ppy..GET /java/
0040  6d 69 64 70 2e 77 6d 6c 20 48 54 54 50 2f 31 2e   midp.wml HTTP/1.
0050  31 0d 0a 54 4d 5f 75 73 65 72 2d 69 64 3a 20 30   1..TM_user-id: 0
0060  33 34 36 30 32 37 33 38 34 33 31 35 34 36 31 33   3460273843154613
0070  30 37 0d 0a 78 2d 75 70 2d 73 75 62 6e 6f 3a 20   07..x-up-subno: 
0080  30 33 34 36 30 32 37 33 38 34 33 31 35 34 36 31   0346027384315461
0090  33 30 37 0d 0a 43 6f 6e 6e 65 63 74 69 6f 6e 3a   307..Connection:
00a0  20 63 6c 6f 73 65 0d 0a 48 6f 73 74 3a 20 31 39    close..Host: 19
00b0  35 2e 32 33 35 2e 31 36 30 2e 38 30 0d 0a 41 63   5.235.160.80..Ac
00c0  63 65 70 74 3a 20 6d 75 6c 74 69 70 61 72 74 2f   cept: multipart/
00d0  6d 69 78 65 64 2c 20 61 70 70 6c 69 63 61 74 69   mixed, applicati
00e0  6f 6e 2f 76 6e 64 2e 77 61 70 2e 6d 75 6c 74 69   on/vnd.wap.multi
00f0  70 61 72 74 2e 6d 69 78 65 64 2c 20 61 70 70 6c   part.mixed, appl
0100  69 63 61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70 2e   ication/vnd.wap.
0110  78 68 74 6d 6c 2b 78 6d 6c 2c 20 61 70 70 6c 69   xhtml+xml, appli
0120  63 61 74 69 6f 6e 2f 78 68 74 6d 6c 2b 78 6d 6c   cation/xhtml+xml
0130  2c 20 74 65 78 74 2f 76 6e 64 2e 77 61 70 2e 77   , text/vnd.wap.w
0140  6d 6c 2c 20 2a 2f 2a 2c 2a 2f 2a 0d 0a 41 63 63   ml, */*,*/*..Acc
0150  65 70 74 2d 43 68 61 72 73 65 74 3a 20 75 74 66   ept-Charset: utf
0160  2d 38 2c 20 75 74 66 2d 31 36 2c 20 69 73 6f 2d   -8, utf-16, iso-
0170  38 38 35 39 2d 31 2c 20 69 73 6f 2d 31 30 36 34   8859-1, iso-1064
0180  36 2d 75 63 73 2d 32 2c 20 53 68 69 66 74 5f 4a   6-ucs-2, Shift_J
0190  49 53 2c 20 42 69 67 35 2c 2a 0d 0a 41 63 63 65   IS, Big5,*..Acce
01a0  70 74 2d 45 6e 63 6f 64 69 6e 67 3a 20 67 7a 69   pt-Encoding: gzi
01b0  70 2c 20 64 65 66 6c 61 74 65 0d 0a 41 63 63 65   p, deflate..Acce
01c0  70 74 2d 4c 61 6e 67 75 61 67 65 3a 20 65 73 0d   pt-Language: es.
01d0  0a 52 65 66 65 72 65 72 3a 20 68 74 74 70 3a 2f   .Referer: http:/
01e0  2f 31 39 35 2e 32 33 35 2e 31 36 30 2e 38 30 2f   /195.235.160.80/
01f0  6a 61 76 61 2f 69 6e 64 65 78 2e 77 6d 6c 0d 0a   java/index.wml..
0200  55 73 65 72 2d 41 67 65 6e 74 3a 20 53 6f 6e 79   User-Agent: Sony
0210  45 72 69 63 73 73 6f 6e 5a 35 33 30 69 2f 52 36   EricssonZ530i/R6
0220  41 43 20 42 72 6f 77 73 65 72 2f 4e 65 74 46 72   AC Browser/NetFr
0230  6f 6e 74 2f 33 2e 33 20 50 72 6f 66 69 6c 65 2f   ont/3.3 Profile/
0240  4d 49 44 50 2d 32 2e 30 20 43 6f 6e 66 69 67 75   MIDP-2.0 Configu
0250  72 61 74 69 6f 6e 2f 43 4c 44 43 2d 31 2e 31 20   ration/CLDC-1.1 
0260  55 50 2e 4c 69 6e 6b 2f 36 2e 32 2e 33 2e 31 35   UP.Link/6.2.3.15
0270  2e 30 0d 0a 78 2d 77 61 70 2d 70 72 6f 66 69 6c   .0..x-wap-profil
0280  65 3a 20 22 68 74 74 70 3a 2f 2f 77 61 70 2e 73   e: "http://wap.s
0290  6f 6e 79 65 72 69 63 73 73 6f 6e 2e 63 6f 6d 2f   onyericsson.com/
02a0  55 41 70 72 6f 66 2f 5a 35 33 30 69 52 32 30 31   UAprof/Z530iR201
02b0  2e 78 6d 6c 22 0d 0a 78 2d 75 70 2d 66 6f 72 77   .xml"..x-up-forw
02c0  61 72 64 65 64 2d 66 6f 72 3a 20 31 30 2e 31 34   arded-for: 10.14
02d0  36 2e 36 33 2e 30 0d 0a 56 69 61 3a 20 31 2e 31   6.63.0..Via: 1.1
02e0  20 6d 62 65 2d 70 72 6f 78 79 32 70 65 2e 77 61    mbe-proxy2pe.wa
02f0  70 2e 6f 6c 65 61 64 61 2e 63 6f 6d 3a 38 30 38   p.oleada.com:808
0300  30 0d 0a 0d 0a                                    0....

Frame 15 (787 bytes on wire, 787 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.643435000
    Time delta from previous packet: 0.000751000 seconds
    Time since reference or first frame: 4.522086000 seconds
    Frame Number: 15
    Packet Length: 787 bytes
    Capture Length: 787 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 773
    Identification: 0x756f (30063)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2bdc)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47671 (47671), Seq: 1, Ack: 720, Len: 733
    Source port: http (80)
    Destination port: 47671 (47671)
    Sequence number: 1
    Next sequence number: 734
    Acknowledgement number: 720
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16801
    Checksum: 0x599f (incorrect, should be 0x0972)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 14
        The RTT to ACK the segment was: 0.000751000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:18 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Mon, 24 Oct 2005 13:19:50 GMT\r\n
    ETag: "0-1e2-435cdf76"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 482\r\n
    Connection: close\r\n
    Content-Type: text/vnd.wap.wml\r\n
    \r\n
    Data (482 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  03 05 75 6f 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..uo@........P.7
0020  2f 34 00 50 ba 37 90 29 41 fe 57 85 9f 3a 50 18   /4.P.7.)A.W..:P.
0030  41 a1 59 9f 00 00 48 54 54 50 2f 31 2e 31 20 32   A.Y...HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 31 38 20 47 4d 54 0d 0a 53 65 72 76   :42:18 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 4d 6f 6e 2c 20 32   Modified: Mon, 2
00a0  34 20 4f 63 74 20 32 30 30 35 20 31 33 3a 31 39   4 Oct 2005 13:19
00b0  3a 35 30 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :50 GMT..ETag: "
00c0  30 2d 31 65 32 2d 34 33 35 63 64 66 37 36 22 0d   0-1e2-435cdf76".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 34 38 32 0d 0a 43 6f 6e 6e   ength: 482..Conn
0100  65 63 74 69 6f 6e 3a 20 63 6c 6f 73 65 0d 0a 43   ection: close..C
0110  6f 6e 74 65 6e 74 2d 54 79 70 65 3a 20 74 65 78   ontent-Type: tex
0120  74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c 0d 0a 0d   t/vnd.wap.wml...
0130  0a 3c 3f 78 6d 6c 20 76 65 72 73 69 6f 6e 3d 22   .<?xml version="
0140  31 2e 30 22 3f 3e 20 0d 0a 3c 21 44 4f 43 54 59   1.0"?> ..<!DOCTY
0150  50 45 20 77 6d 6c 20 50 55 42 4c 49 43 20 22 2d   PE wml PUBLIC "-
0160  2f 2f 57 41 50 46 4f 52 55 4d 2f 2f 44 54 44 20   //WAPFORUM//DTD 
0170  57 4d 4c 20 31 2e 31 2f 2f 45 4e 22 20 22 68 74   WML 1.1//EN" "ht
0180  74 70 3a 2f 2f 77 77 77 2e 77 61 70 66 6f 72 75   tp://www.wapforu
0190  6d 2e 6f 72 67 2f 44 54 44 2f 77 6d 6c 5f 31 2e   m.org/DTD/wml_1.
01a0  31 2e 78 6d 6c 22 3e 20 0d 0a 0d 0a 3c 77 6d 6c   1.xml"> ....<wml
01b0  3e 0d 0a 0d 0a 3c 68 65 61 64 3e 20 0d 0a 3c 6d   >....<head> ..<m
01c0  65 74 61 20 68 74 74 70 2d 65 71 75 69 76 3d 22   eta http-equiv="
01d0  43 6f 6e 74 65 6e 74 2d 54 79 70 65 22 20 63 6f   Content-Type" co
01e0  6e 74 65 6e 74 3d 22 74 65 78 74 2f 76 6e 64 2e   ntent="text/vnd.
01f0  77 61 70 2e 77 6d 6c 3b 20 63 68 61 72 73 65 74   wap.wml; charset
0200  3d 69 73 6f 2d 38 38 35 39 2d 31 22 2f 3e 0d 0a   =iso-8859-1"/>..
0210  3c 2f 68 65 61 64 3e 0d 0a 0d 0a 3c 63 61 72 64   </head>....<card
0220  20 74 69 74 6c 65 3d 22 4d 49 44 50 20 69 6e 64    title="MIDP ind
0230  65 78 22 3e 0d 0a 20 3c 70 3e 0d 0a 20 20 4d 49   ex">.. <p>..  MI
0240  44 50 20 6d 65 6e 75 3a 20 3c 62 72 2f 3e 0d 0a   DP menu: <br/>..
0250  20 20 3c 61 20 68 72 65 66 3d 22 69 6e 64 65 78     <a href="index
0260  5f 74 6d 65 2e 77 6d 6c 22 3e 26 67 74 3b 54 4d   _tme.wml">&gt;TM
0270  45 20 74 65 73 74 73 3c 2f 61 3e 3c 62 72 2f 3e   E tests</a><br/>
0280  0d 0a 20 20 3c 21 2d 2d 20 20 3c 61 20 68 72 65   ..  <!--  <a hre
0290  66 3d 22 2e 2e 2f 6d 74 65 2f 63 67 69 2d 62 69   f="../mte/cgi-bi
02a0  6e 2f 77 6d 6c 2e 63 67 69 22 3e 26 67 74 3b 4d   n/wml.cgi">&gt;M
02b0  54 45 20 74 65 73 74 73 3c 2f 61 3e 3c 62 72 2f   TE tests</a><br/
02c0  3e 20 2d 2d 3e 0d 0a 20 20 3c 61 20 68 72 65 66   > -->..  <a href
02d0  3d 22 66 61 62 72 69 63 61 6e 74 65 73 2e 77 6d   ="fabricantes.wm
02e0  6c 22 3e 26 67 74 3b 4d 54 45 20 74 65 73 74 73   l">&gt;MTE tests
02f0  3c 2f 61 3e 3c 62 72 2f 3e 0d 0a 20 3c 2f 70 3e   </a><br/>.. </p>
0300  0d 0a 3c 2f 63 61 72 64 3e 0d 0a 0d 0a 3c 2f 77   ..</card>....</w
0310  6d 6c 3e                                          ml>

Frame 16 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.643482000
    Time delta from previous packet: 0.000047000 seconds
    Time since reference or first frame: 4.522133000 seconds
    Frame Number: 16
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x7570 (30064)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eb8)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47671 (47671), Seq: 734, Ack: 720, Len: 0
    Source port: http (80)
    Destination port: 47671 (47671)
    Sequence number: 734
    Acknowledgement number: 720
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16801
    Checksum: 0x56c2 (incorrect, should be 0x913e)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 70 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(up@........P.7
0020  2f 34 00 50 ba 37 90 29 44 db 57 85 9f 3a 50 11   /4.P.7.)D.W..:P.
0030  41 a1 56 c2 00 00                                 A.V...

Frame 17 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.644140000
    Time delta from previous packet: 0.000658000 seconds
    Time since reference or first frame: 4.522791000 seconds
    Frame Number: 17
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x99ea (39402)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x4a3e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47671 (47671), Dst Port: http (80), Seq: 720, Ack: 734, Len: 0
    Source port: 47671 (47671)
    Destination port: http (80)
    Sequence number: 720
    Acknowledgement number: 734
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6597
    Checksum: 0xb91b (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 15
        The RTT to ACK the segment was: 0.000705000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 99 ea 40 00 40 06 4a 3e c3 37 2f 34 c3 eb   .(..@.@.J>.7/4..
0020  a0 50 ba 37 00 50 57 85 9f 3a 90 29 44 db 50 10   .P.7.PW..:.)D.P.
0030  19 c5 b9 1b 00 00 00 00 00 00 00 00               ............

Frame 18 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.649733000
    Time delta from previous packet: 0.005593000 seconds
    Time since reference or first frame: 4.528384000 seconds
    Frame Number: 18
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x99eb (39403)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x4a3d (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47671 (47671), Dst Port: http (80), Seq: 720, Ack: 735, Len: 0
    Source port: 47671 (47671)
    Destination port: http (80)
    Sequence number: 720
    Acknowledgement number: 735
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6597
    Checksum: 0xb919 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 16
        The RTT to ACK the segment was: 0.006251000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 99 eb 40 00 40 06 4a 3d c3 37 2f 34 c3 eb   .(..@.@.J=.7/4..
0020  a0 50 ba 37 00 50 57 85 9f 3a 90 29 44 dc 50 11   .P.7.PW..:.)D.P.
0030  19 c5 b9 19 00 00 00 00 00 00 00 00               ............

Frame 19 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:18.649741000
    Time delta from previous packet: 0.000008000 seconds
    Time since reference or first frame: 4.528392000 seconds
    Frame Number: 19
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x7571 (30065)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eb7)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47671 (47671), Seq: 735, Ack: 721, Len: 0
    Source port: http (80)
    Destination port: 47671 (47671)
    Sequence number: 735
    Acknowledgement number: 721
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16801
    Checksum: 0x56c2 (incorrect, should be 0x913d)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 18
        The RTT to ACK the segment was: 0.000008000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 71 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(uq@........P.7
0020  2f 34 00 50 ba 37 90 29 44 dc 57 85 9f 3b 50 10   /4.P.7.)D.W..;P.
0030  41 a1 56 c2 00 00                                 A.V...

Frame 20 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.056990000
    Time delta from previous packet: 6.407249000 seconds
    Time since reference or first frame: 10.935641000 seconds
    Frame Number: 20
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7c85 (31877)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0x6b3b (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47907 (47907), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 47907 (47907)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x0cbd (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 7c 85 40 00 3c 06 6b 3b c3 37 2f 34 c3 eb   .0|.@.<.k;.7/4..
0020  a0 50 bb 23 00 50 70 a2 92 b0 00 00 00 00 70 02   .P.#.Pp.......p.
0030  60 f4 0c bd 00 00 02 04 05 b4 01 01 04 02         `.............

Frame 21 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.057027000
    Time delta from previous packet: 0.000037000 seconds
    Time since reference or first frame: 10.935678000 seconds
    Frame Number: 21
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7572 (30066)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eae)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47907 (47907), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 47907 (47907)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x766a (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 20
        The RTT to ACK the segment was: 0.000037000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 72 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0ur@........P.7
0020  2f 34 00 50 bb 23 7f d8 32 ed 70 a2 92 b1 70 12   /4.P.#..2.p...p.
0030  44 70 76 6a 00 00 02 04 05 b4 01 01 04 02         Dpvj..........

Frame 22 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.115594000
    Time delta from previous packet: 0.058567000 seconds
    Time since reference or first frame: 10.994245000 seconds
    Frame Number: 22
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xd3ed (54253)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x103b (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47907 (47907), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 47907 (47907)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xd22e (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 21
        The RTT to ACK the segment was: 0.058567000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 d3 ed 40 00 40 06 10 3b c3 37 2f 34 c3 eb   .(..@.@..;.7/4..
0020  a0 50 bb 23 00 50 70 a2 92 b1 7f d8 32 ee 50 10   .P.#.Pp.....2.P.
0030  15 70 d2 2e 00 00 00 00 00 00 00 00               .p..........

Frame 23 (777 bytes on wire, 777 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.132377000
    Time delta from previous packet: 0.016783000 seconds
    Time since reference or first frame: 11.011028000 seconds
    Frame Number: 23
    Packet Length: 777 bytes
    Capture Length: 777 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 763
    Identification: 0xd3ee (54254)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x0d67 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47907 (47907), Dst Port: http (80), Seq: 1, Ack: 1, Len: 723
    Source port: 47907 (47907)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 724
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x550b (correct)
Hypertext Transfer Protocol
    GET /java/index_tme.wml HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Connection: close\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/java/midp.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  02 fb d3 ee 40 00 40 06 0d 67 c3 37 2f 34 c3 eb   ....@.@..g.7/4..
0020  a0 50 bb 23 00 50 70 a2 92 b1 7f d8 32 ee 50 18   .P.#.Pp.....2.P.
0030  15 70 55 0b 00 00 47 45 54 20 2f 6a 61 76 61 2f   .pU...GET /java/
0040  69 6e 64 65 78 5f 74 6d 65 2e 77 6d 6c 20 48 54   index_tme.wml HT
0050  54 50 2f 31 2e 31 0d 0a 54 4d 5f 75 73 65 72 2d   TP/1.1..TM_user-
0060  69 64 3a 20 30 33 34 36 30 32 37 33 38 34 33 31   id: 034602738431
0070  35 34 36 31 33 30 37 0d 0a 78 2d 75 70 2d 73 75   5461307..x-up-su
0080  62 6e 6f 3a 20 30 33 34 36 30 32 37 33 38 34 33   bno: 03460273843
0090  31 35 34 36 31 33 30 37 0d 0a 43 6f 6e 6e 65 63   15461307..Connec
00a0  74 69 6f 6e 3a 20 63 6c 6f 73 65 0d 0a 48 6f 73   tion: close..Hos
00b0  74 3a 20 31 39 35 2e 32 33 35 2e 31 36 30 2e 38   t: 195.235.160.8
00c0  30 0d 0a 41 63 63 65 70 74 3a 20 6d 75 6c 74 69   0..Accept: multi
00d0  70 61 72 74 2f 6d 69 78 65 64 2c 20 61 70 70 6c   part/mixed, appl
00e0  69 63 61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70 2e   ication/vnd.wap.
00f0  6d 75 6c 74 69 70 61 72 74 2e 6d 69 78 65 64 2c   multipart.mixed,
0100  20 61 70 70 6c 69 63 61 74 69 6f 6e 2f 76 6e 64    application/vnd
0110  2e 77 61 70 2e 78 68 74 6d 6c 2b 78 6d 6c 2c 20   .wap.xhtml+xml, 
0120  61 70 70 6c 69 63 61 74 69 6f 6e 2f 78 68 74 6d   application/xhtm
0130  6c 2b 78 6d 6c 2c 20 74 65 78 74 2f 76 6e 64 2e   l+xml, text/vnd.
0140  77 61 70 2e 77 6d 6c 2c 20 2a 2f 2a 2c 2a 2f 2a   wap.wml, */*,*/*
0150  0d 0a 41 63 63 65 70 74 2d 43 68 61 72 73 65 74   ..Accept-Charset
0160  3a 20 75 74 66 2d 38 2c 20 75 74 66 2d 31 36 2c   : utf-8, utf-16,
0170  20 69 73 6f 2d 38 38 35 39 2d 31 2c 20 69 73 6f    iso-8859-1, iso
0180  2d 31 30 36 34 36 2d 75 63 73 2d 32 2c 20 53 68   -10646-ucs-2, Sh
0190  69 66 74 5f 4a 49 53 2c 20 42 69 67 35 2c 2a 0d   ift_JIS, Big5,*.
01a0  0a 41 63 63 65 70 74 2d 45 6e 63 6f 64 69 6e 67   .Accept-Encoding
01b0  3a 20 67 7a 69 70 2c 20 64 65 66 6c 61 74 65 0d   : gzip, deflate.
01c0  0a 41 63 63 65 70 74 2d 4c 61 6e 67 75 61 67 65   .Accept-Language
01d0  3a 20 65 73 0d 0a 52 65 66 65 72 65 72 3a 20 68   : es..Referer: h
01e0  74 74 70 3a 2f 2f 31 39 35 2e 32 33 35 2e 31 36   ttp://195.235.16
01f0  30 2e 38 30 2f 6a 61 76 61 2f 6d 69 64 70 2e 77   0.80/java/midp.w
0200  6d 6c 0d 0a 55 73 65 72 2d 41 67 65 6e 74 3a 20   ml..User-Agent: 
0210  53 6f 6e 79 45 72 69 63 73 73 6f 6e 5a 35 33 30   SonyEricssonZ530
0220  69 2f 52 36 41 43 20 42 72 6f 77 73 65 72 2f 4e   i/R6AC Browser/N
0230  65 74 46 72 6f 6e 74 2f 33 2e 33 20 50 72 6f 66   etFront/3.3 Prof
0240  69 6c 65 2f 4d 49 44 50 2d 32 2e 30 20 43 6f 6e   ile/MIDP-2.0 Con
0250  66 69 67 75 72 61 74 69 6f 6e 2f 43 4c 44 43 2d   figuration/CLDC-
0260  31 2e 31 20 55 50 2e 4c 69 6e 6b 2f 36 2e 32 2e   1.1 UP.Link/6.2.
0270  33 2e 31 35 2e 30 0d 0a 78 2d 77 61 70 2d 70 72   3.15.0..x-wap-pr
0280  6f 66 69 6c 65 3a 20 22 68 74 74 70 3a 2f 2f 77   ofile: "http://w
0290  61 70 2e 73 6f 6e 79 65 72 69 63 73 73 6f 6e 2e   ap.sonyericsson.
02a0  63 6f 6d 2f 55 41 70 72 6f 66 2f 5a 35 33 30 69   com/UAprof/Z530i
02b0  52 32 30 31 2e 78 6d 6c 22 0d 0a 78 2d 75 70 2d   R201.xml"..x-up-
02c0  66 6f 72 77 61 72 64 65 64 2d 66 6f 72 3a 20 31   forwarded-for: 1
02d0  30 2e 31 34 36 2e 36 33 2e 30 0d 0a 56 69 61 3a   0.146.63.0..Via:
02e0  20 31 2e 31 20 6d 62 65 2d 70 72 6f 78 79 32 70    1.1 mbe-proxy2p
02f0  65 2e 77 61 70 2e 6f 6c 65 61 64 61 2e 63 6f 6d   e.wap.oleada.com
0300  3a 38 30 38 30 0d 0a 0d 0a                        :8080....

Frame 24 (802 bytes on wire, 802 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.133124000
    Time delta from previous packet: 0.000747000 seconds
    Time since reference or first frame: 11.011775000 seconds
    Frame Number: 24
    Packet Length: 802 bytes
    Capture Length: 802 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 788
    Identification: 0x7573 (30067)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2bc9)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47907 (47907), Seq: 1, Ack: 724, Len: 748
    Source port: http (80)
    Destination port: 47907 (47907)
    Sequence number: 1
    Next sequence number: 749
    Acknowledgement number: 724
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16797
    Checksum: 0x59ae (incorrect, should be 0x7021)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 23
        The RTT to ACK the segment was: 0.000747000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:25 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Mon, 07 Nov 2005 11:30:00 GMT\r\n
    ETag: "0-1f1-436f3ab8"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 497\r\n
    Connection: close\r\n
    Content-Type: text/vnd.wap.wml\r\n
    \r\n
    Data (497 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  03 14 75 73 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..us@........P.7
0020  2f 34 00 50 bb 23 7f d8 32 ee 70 a2 95 84 50 18   /4.P.#..2.p...P.
0030  41 9d 59 ae 00 00 48 54 54 50 2f 31 2e 31 20 32   A.Y...HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 32 35 20 47 4d 54 0d 0a 53 65 72 76   :42:25 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 4d 6f 6e 2c 20 30   Modified: Mon, 0
00a0  37 20 4e 6f 76 20 32 30 30 35 20 31 31 3a 33 30   7 Nov 2005 11:30
00b0  3a 30 30 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :00 GMT..ETag: "
00c0  30 2d 31 66 31 2d 34 33 36 66 33 61 62 38 22 0d   0-1f1-436f3ab8".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 34 39 37 0d 0a 43 6f 6e 6e   ength: 497..Conn
0100  65 63 74 69 6f 6e 3a 20 63 6c 6f 73 65 0d 0a 43   ection: close..C
0110  6f 6e 74 65 6e 74 2d 54 79 70 65 3a 20 74 65 78   ontent-Type: tex
0120  74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c 0d 0a 0d   t/vnd.wap.wml...
0130  0a 3c 3f 78 6d 6c 20 76 65 72 73 69 6f 6e 3d 22   .<?xml version="
0140  31 2e 30 22 3f 3e 20 0d 0a 3c 21 44 4f 43 54 59   1.0"?> ..<!DOCTY
0150  50 45 20 77 6d 6c 20 50 55 42 4c 49 43 20 22 2d   PE wml PUBLIC "-
0160  2f 2f 57 41 50 46 4f 52 55 4d 2f 2f 44 54 44 20   //WAPFORUM//DTD 
0170  57 4d 4c 20 31 2e 31 2f 2f 45 4e 22 20 22 68 74   WML 1.1//EN" "ht
0180  74 70 3a 2f 2f 77 77 77 2e 77 61 70 66 6f 72 75   tp://www.wapforu
0190  6d 2e 6f 72 67 2f 44 54 44 2f 77 6d 6c 5f 31 2e   m.org/DTD/wml_1.
01a0  31 2e 78 6d 6c 22 3e 20 0d 0a 0d 0a 3c 77 6d 6c   1.xml"> ....<wml
01b0  3e 0d 0a 0d 0a 3c 68 65 61 64 3e 20 0d 0a 3c 6d   >....<head> ..<m
01c0  65 74 61 20 68 74 74 70 2d 65 71 75 69 76 3d 22   eta http-equiv="
01d0  43 6f 6e 74 65 6e 74 2d 54 79 70 65 22 20 63 6f   Content-Type" co
01e0  6e 74 65 6e 74 3d 22 74 65 78 74 2f 76 6e 64 2e   ntent="text/vnd.
01f0  77 61 70 2e 77 6d 6c 3b 20 63 68 61 72 73 65 74   wap.wml; charset
0200  3d 69 73 6f 2d 38 38 35 39 2d 31 22 2f 3e 0d 0a   =iso-8859-1"/>..
0210  3c 2f 68 65 61 64 3e 0d 0a 0d 0a 3c 63 61 72 64   </head>....<card
0220  20 74 69 74 6c 65 3d 22 54 4d 45 20 74 65 73 74    title="TME test
0230  73 22 3e 0d 0a 20 3c 70 3e 0d 0a 20 20 4d 49 44   s">.. <p>..  MID
0240  50 20 74 65 73 74 73 3a 20 3c 62 72 2f 3e 0d 0a   P tests: <br/>..
0250  20 20 3c 61 20 68 72 65 66 3d 22 2e 2f 6d 69 64     <a href="./mid
0260  70 31 30 2f 69 6e 64 65 78 5f 6d 69 64 70 31 2e   p10/index_midp1.
0270  77 6d 6c 22 3e 26 67 74 3b 4d 49 44 50 20 31 2e   wml">&gt;MIDP 1.
0280  30 3c 2f 61 3e 3c 62 72 2f 3e 0d 0a 20 20 3c 61   0</a><br/>..  <a
0290  20 68 72 65 66 3d 22 2e 2f 6d 69 64 70 32 30 2f    href="./midp20/
02a0  69 6e 64 65 78 5f 6d 69 64 70 32 2e 77 6d 6c 22   index_midp2.wml"
02b0  3e 26 67 74 3b 4d 49 44 50 20 32 2e 30 3c 2f 61   >&gt;MIDP 2.0</a
02c0  3e 3c 62 72 2f 3e 0d 0a 20 20 3c 61 20 68 72 65   ><br/>..  <a hre
02d0  66 3d 22 2e 2f 73 70 65 63 69 61 6c 5f 4a 53 52   f="./special_JSR
02e0  2f 69 6e 64 65 78 5f 6a 73 72 2e 77 6d 6c 22 3e   /index_jsr.wml">
02f0  26 67 74 3b 73 70 65 63 69 61 6c 5f 4a 53 52 3c   &gt;special_JSR<
0300  2f 61 3e 3c 62 72 2f 3e 0d 0a 20 3c 2f 70 3e 0d   /a><br/>.. </p>.
0310  0a 3c 2f 63 61 72 64 3e 0d 0a 0d 0a 3c 2f 77 6d   .</card>....</wm
0320  6c 3e                                             l>

Frame 25 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.133171000
    Time delta from previous packet: 0.000047000 seconds
    Time since reference or first frame: 11.011822000 seconds
    Frame Number: 25
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x7574 (30068)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eb4)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47907 (47907), Seq: 749, Ack: 724, Len: 0
    Source port: http (80)
    Destination port: 47907 (47907)
    Sequence number: 749
    Acknowledgement number: 724
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16797
    Checksum: 0x56c2 (incorrect, should be 0xa041)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 74 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(ut@........P.7
0020  2f 34 00 50 bb 23 7f d8 35 da 70 a2 95 84 50 11   /4.P.#..5.p...P.
0030  41 9d 56 c2 00 00                                 A.V...

Frame 26 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.133831000
    Time delta from previous packet: 0.000660000 seconds
    Time since reference or first frame: 11.012482000 seconds
    Frame Number: 26
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xd3ef (54255)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x1039 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47907 (47907), Dst Port: http (80), Seq: 724, Ack: 749, Len: 0
    Source port: 47907 (47907)
    Destination port: http (80)
    Sequence number: 724
    Acknowledgement number: 749
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6732
    Checksum: 0xc793 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 24
        The RTT to ACK the segment was: 0.000707000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 d3 ef 40 00 40 06 10 39 c3 37 2f 34 c3 eb   .(..@.@..9.7/4..
0020  a0 50 bb 23 00 50 70 a2 95 84 7f d8 35 da 50 10   .P.#.Pp.....5.P.
0030  1a 4c c7 93 00 00 00 00 00 00 00 00               .L..........

Frame 27 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.135045000
    Time delta from previous packet: 0.001214000 seconds
    Time since reference or first frame: 11.013696000 seconds
    Frame Number: 27
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xd3f0 (54256)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x1038 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 47907 (47907), Dst Port: http (80), Seq: 724, Ack: 750, Len: 0
    Source port: 47907 (47907)
    Destination port: http (80)
    Sequence number: 724
    Acknowledgement number: 750
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6732
    Checksum: 0xc791 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 25
        The RTT to ACK the segment was: 0.001874000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 d3 f0 40 00 40 06 10 38 c3 37 2f 34 c3 eb   .(..@.@..8.7/4..
0020  a0 50 bb 23 00 50 70 a2 95 84 7f d8 35 db 50 11   .P.#.Pp.....5.P.
0030  1a 4c c7 91 00 00 00 00 00 00 00 00               .L..........

Frame 28 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:25.135053000
    Time delta from previous packet: 0.000008000 seconds
    Time since reference or first frame: 11.013704000 seconds
    Frame Number: 28
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x7575 (30069)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eb3)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 47907 (47907), Seq: 750, Ack: 725, Len: 0
    Source port: http (80)
    Destination port: 47907 (47907)
    Sequence number: 750
    Acknowledgement number: 725
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16797
    Checksum: 0x56c2 (incorrect, should be 0xa040)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 27
        The RTT to ACK the segment was: 0.000008000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 75 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(uu@........P.7
0020  2f 34 00 50 bb 23 7f d8 35 db 70 a2 95 85 50 10   /4.P.#..5.p...P.
0030  41 9d 56 c2 00 00                                 A.V...

Frame 29 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.123818000
    Time delta from previous packet: 2.988765000 seconds
    Time since reference or first frame: 14.002469000 seconds
    Frame Number: 29
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0xefeb (61419)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xf7d4 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48021 (48021), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 48021 (48021)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x410d (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 ef eb 40 00 3c 06 f7 d4 c3 37 2f 34 c3 eb   .0..@.<....7/4..
0020  a0 50 bb 95 00 50 fc fa d1 95 00 00 00 00 70 02   .P...P........p.
0030  60 f4 41 0d 00 00 02 04 05 b4 01 01 04 02         `.A...........

Frame 30 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.123850000
    Time delta from previous packet: 0.000032000 seconds
    Time since reference or first frame: 14.002501000 seconds
    Frame Number: 30
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7576 (30070)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eaa)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48021 (48021), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 48021 (48021)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x3e50 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 29
        The RTT to ACK the segment was: 0.000032000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 76 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0uv@........P.7
0020  2f 34 00 50 bb 95 bd 25 62 0a fc fa d1 96 70 12   /4.P...%b.....p.
0030  44 70 3e 50 00 00 02 04 05 b4 01 01 04 02         Dp>P..........

Frame 31 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.172465000
    Time delta from previous packet: 0.048615000 seconds
    Time since reference or first frame: 14.051116000 seconds
    Frame Number: 31
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x74b7 (29879)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x6f71 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48021 (48021), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 48021 (48021)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x9a14 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 30
        The RTT to ACK the segment was: 0.048615000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 74 b7 40 00 40 06 6f 71 c3 37 2f 34 c3 eb   .(t.@.@.oq.7/4..
0020  a0 50 bb 95 00 50 fc fa d1 96 bd 25 62 0b 50 10   .P...P.....%b.P.
0030  15 70 9a 14 00 00 00 00 00 00 00 00               .p..........

Frame 32 (791 bytes on wire, 791 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.175376000
    Time delta from previous packet: 0.002911000 seconds
    Time since reference or first frame: 14.054027000 seconds
    Frame Number: 32
    Packet Length: 791 bytes
    Capture Length: 791 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 777
    Identification: 0x74b8 (29880)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x6c8f (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48021 (48021), Dst Port: http (80), Seq: 1, Ack: 1, Len: 737
    Source port: 48021 (48021)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 738
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x0d0c (correct)
Hypertext Transfer Protocol
    GET /java/midp10/index_midp1.wml HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Connection: close\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/java/index_tme.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  03 09 74 b8 40 00 40 06 6c 8f c3 37 2f 34 c3 eb   ..t.@.@.l..7/4..
0020  a0 50 bb 95 00 50 fc fa d1 96 bd 25 62 0b 50 18   .P...P.....%b.P.
0030  15 70 0d 0c 00 00 47 45 54 20 2f 6a 61 76 61 2f   .p....GET /java/
0040  6d 69 64 70 31 30 2f 69 6e 64 65 78 5f 6d 69 64   midp10/index_mid
0050  70 31 2e 77 6d 6c 20 48 54 54 50 2f 31 2e 31 0d   p1.wml HTTP/1.1.
0060  0a 54 4d 5f 75 73 65 72 2d 69 64 3a 20 30 33 34   .TM_user-id: 034
0070  36 30 32 37 33 38 34 33 31 35 34 36 31 33 30 37   6027384315461307
0080  0d 0a 78 2d 75 70 2d 73 75 62 6e 6f 3a 20 30 33   ..x-up-subno: 03
0090  34 36 30 32 37 33 38 34 33 31 35 34 36 31 33 30   4602738431546130
00a0  37 0d 0a 43 6f 6e 6e 65 63 74 69 6f 6e 3a 20 63   7..Connection: c
00b0  6c 6f 73 65 0d 0a 48 6f 73 74 3a 20 31 39 35 2e   lose..Host: 195.
00c0  32 33 35 2e 31 36 30 2e 38 30 0d 0a 41 63 63 65   235.160.80..Acce
00d0  70 74 3a 20 6d 75 6c 74 69 70 61 72 74 2f 6d 69   pt: multipart/mi
00e0  78 65 64 2c 20 61 70 70 6c 69 63 61 74 69 6f 6e   xed, application
00f0  2f 76 6e 64 2e 77 61 70 2e 6d 75 6c 74 69 70 61   /vnd.wap.multipa
0100  72 74 2e 6d 69 78 65 64 2c 20 61 70 70 6c 69 63   rt.mixed, applic
0110  61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70 2e 78 68   ation/vnd.wap.xh
0120  74 6d 6c 2b 78 6d 6c 2c 20 61 70 70 6c 69 63 61   tml+xml, applica
0130  74 69 6f 6e 2f 78 68 74 6d 6c 2b 78 6d 6c 2c 20   tion/xhtml+xml, 
0140  74 65 78 74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c   text/vnd.wap.wml
0150  2c 20 2a 2f 2a 2c 2a 2f 2a 0d 0a 41 63 63 65 70   , */*,*/*..Accep
0160  74 2d 43 68 61 72 73 65 74 3a 20 75 74 66 2d 38   t-Charset: utf-8
0170  2c 20 75 74 66 2d 31 36 2c 20 69 73 6f 2d 38 38   , utf-16, iso-88
0180  35 39 2d 31 2c 20 69 73 6f 2d 31 30 36 34 36 2d   59-1, iso-10646-
0190  75 63 73 2d 32 2c 20 53 68 69 66 74 5f 4a 49 53   ucs-2, Shift_JIS
01a0  2c 20 42 69 67 35 2c 2a 0d 0a 41 63 63 65 70 74   , Big5,*..Accept
01b0  2d 45 6e 63 6f 64 69 6e 67 3a 20 67 7a 69 70 2c   -Encoding: gzip,
01c0  20 64 65 66 6c 61 74 65 0d 0a 41 63 63 65 70 74    deflate..Accept
01d0  2d 4c 61 6e 67 75 61 67 65 3a 20 65 73 0d 0a 52   -Language: es..R
01e0  65 66 65 72 65 72 3a 20 68 74 74 70 3a 2f 2f 31   eferer: http://1
01f0  39 35 2e 32 33 35 2e 31 36 30 2e 38 30 2f 6a 61   95.235.160.80/ja
0200  76 61 2f 69 6e 64 65 78 5f 74 6d 65 2e 77 6d 6c   va/index_tme.wml
0210  0d 0a 55 73 65 72 2d 41 67 65 6e 74 3a 20 53 6f   ..User-Agent: So
0220  6e 79 45 72 69 63 73 73 6f 6e 5a 35 33 30 69 2f   nyEricssonZ530i/
0230  52 36 41 43 20 42 72 6f 77 73 65 72 2f 4e 65 74   R6AC Browser/Net
0240  46 72 6f 6e 74 2f 33 2e 33 20 50 72 6f 66 69 6c   Front/3.3 Profil
0250  65 2f 4d 49 44 50 2d 32 2e 30 20 43 6f 6e 66 69   e/MIDP-2.0 Confi
0260  67 75 72 61 74 69 6f 6e 2f 43 4c 44 43 2d 31 2e   guration/CLDC-1.
0270  31 20 55 50 2e 4c 69 6e 6b 2f 36 2e 32 2e 33 2e   1 UP.Link/6.2.3.
0280  31 35 2e 30 0d 0a 78 2d 77 61 70 2d 70 72 6f 66   15.0..x-wap-prof
0290  69 6c 65 3a 20 22 68 74 74 70 3a 2f 2f 77 61 70   ile: "http://wap
02a0  2e 73 6f 6e 79 65 72 69 63 73 73 6f 6e 2e 63 6f   .sonyericsson.co
02b0  6d 2f 55 41 70 72 6f 66 2f 5a 35 33 30 69 52 32   m/UAprof/Z530iR2
02c0  30 31 2e 78 6d 6c 22 0d 0a 78 2d 75 70 2d 66 6f   01.xml"..x-up-fo
02d0  72 77 61 72 64 65 64 2d 66 6f 72 3a 20 31 30 2e   rwarded-for: 10.
02e0  31 34 36 2e 36 33 2e 30 0d 0a 56 69 61 3a 20 31   146.63.0..Via: 1
02f0  2e 31 20 6d 62 65 2d 70 72 6f 78 79 32 70 65 2e   .1 mbe-proxy2pe.
0300  77 61 70 2e 6f 6c 65 61 64 61 2e 63 6f 6d 3a 38   wap.oleada.com:8
0310  30 38 30 0d 0a 0d 0a                              080....

Frame 33 (1514 bytes on wire, 1514 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.176202000
    Time delta from previous packet: 0.000826000 seconds
    Time since reference or first frame: 14.054853000 seconds
    Frame Number: 33
    Packet Length: 1514 bytes
    Capture Length: 1514 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 1500
    Identification: 0x7577 (30071)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x28fd)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48021 (48021), Seq: 1, Ack: 738, Len: 1460
    Source port: http (80)
    Destination port: 48021 (48021)
    Sequence number: 1
    Next sequence number: 1461
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x5c76 (incorrect, should be 0x5c33)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 32
        The RTT to ACK the segment was: 0.000826000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:28 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Mon, 03 Apr 2006 10:03:32 GMT\r\n
    ETag: "0-4c3-4430f2f4"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 1219\r\n
    Connection: close\r\n
    Content-Type: text/vnd.wap.wml\r\n
    \r\n
    Data (1208 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  05 dc 75 77 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..uw@........P.7
0020  2f 34 00 50 bb 95 bd 25 62 0b fc fa d4 77 50 10   /4.P...%b....wP.
0030  41 8f 5c 76 00 00 48 54 54 50 2f 31 2e 31 20 32   A.\v..HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 32 38 20 47 4d 54 0d 0a 53 65 72 76   :42:28 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 4d 6f 6e 2c 20 30   Modified: Mon, 0
00a0  33 20 41 70 72 20 32 30 30 36 20 31 30 3a 30 33   3 Apr 2006 10:03
00b0  3a 33 32 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :32 GMT..ETag: "
00c0  30 2d 34 63 33 2d 34 34 33 30 66 32 66 34 22 0d   0-4c3-4430f2f4".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 31 32 31 39 0d 0a 43 6f 6e   ength: 1219..Con
0100  6e 65 63 74 69 6f 6e 3a 20 63 6c 6f 73 65 0d 0a   nection: close..
0110  43 6f 6e 74 65 6e 74 2d 54 79 70 65 3a 20 74 65   Content-Type: te
0120  78 74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c 0d 0a   xt/vnd.wap.wml..
0130  0d 0a 3c 3f 78 6d 6c 20 76 65 72 73 69 6f 6e 3d   ..<?xml version=
0140  22 31 2e 30 22 3f 3e 20 0d 0a 3c 21 44 4f 43 54   "1.0"?> ..<!DOCT
0150  59 50 45 20 77 6d 6c 20 50 55 42 4c 49 43 20 22   YPE wml PUBLIC "
0160  2d 2f 2f 57 41 50 46 4f 52 55 4d 2f 2f 44 54 44   -//WAPFORUM//DTD
0170  20 57 4d 4c 20 31 2e 31 2f 2f 45 4e 22 20 22 68    WML 1.1//EN" "h
0180  74 74 70 3a 2f 2f 77 77 77 2e 77 61 70 66 6f 72   ttp://www.wapfor
0190  75 6d 2e 6f 72 67 2f 44 54 44 2f 77 6d 6c 5f 31   um.org/DTD/wml_1
01a0  2e 31 2e 78 6d 6c 22 3e 20 0d 0a 3c 77 6d 6c 3e   .1.xml"> ..<wml>
01b0  0d 0a 3c 68 65 61 64 3e 20 0d 0a 3c 6d 65 74 61   ..<head> ..<meta
01c0  20 68 74 74 70 2d 65 71 75 69 76 3d 22 43 6f 6e    http-equiv="Con
01d0  74 65 6e 74 2d 54 79 70 65 22 20 63 6f 6e 74 65   tent-Type" conte
01e0  6e 74 3d 22 74 65 78 74 2f 76 6e 64 2e 77 61 70   nt="text/vnd.wap
01f0  2e 77 6d 6c 3b 20 63 68 61 72 73 65 74 3d 69 73   .wml; charset=is
0200  6f 2d 38 38 35 39 2d 31 22 2f 3e 0d 0a 3c 2f 68   o-8859-1"/>..</h
0210  65 61 64 3e 0d 0a 3c 63 61 72 64 20 74 69 74 6c   ead>..<card titl
0220  65 3d 22 4d 49 44 50 20 31 2e 30 20 54 65 73 74   e="MIDP 1.0 Test
0230  22 3e 0d 0a 0d 0a 3c 70 20 61 6c 69 67 6e 3d 22   ">....<p align="
0240  6c 65 66 74 22 3e 0d 0a 4d 49 44 6c 65 74 73 20   left">..MIDlets 
0250  75 73 65 64 20 74 6f 20 63 68 65 63 6b 20 74 68   used to check th
0260  65 20 4a 32 4d 45 20 63 6c 69 65 6e 74 20 6f 66   e J2ME client of
0270  20 4d 49 44 50 20 31 2e 30 20 64 65 76 69 63 65    MIDP 1.0 device
0280  73 20 3c 62 72 2f 3e 0d 0a 0d 0a 0d 0a 0d 0a 09   s <br/>.........
0290  3c 61 20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65   <a href="./midle
02a0  74 73 2f 4d 49 44 6c 65 74 5f 43 31 2e 6a 61 64   ts/MIDlet_C1.jad
02b0  22 3e 48 54 54 50 20 63 6f 6e 6e 65 63 74 69 6f   ">HTTP connectio
02c0  6e 73 3c 2f 61 3e 28 3c 61 20 68 72 65 66 3d 22   ns</a>(<a href="
02d0  2e 2f 69 6e 66 6f 2f 68 74 74 70 5f 63 6f 6e 6e   ./info/http_conn
02e0  65 63 74 69 6f 6e 73 2e 77 6d 6c 22 3e 69 6e 66   ections.wml">inf
02f0  6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c 61   o</a>)<br/>...<a
0300  20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74 73    href="./midlets
0310  2f 4d 49 44 6c 65 74 5f 43 32 2e 6a 61 64 22 3e   /MIDlet_C2.jad">
0320  4d 49 44 6c 65 74 20 4a 41 52 20 53 69 7a 65 3c   MIDlet JAR Size<
0330  2f 61 3e 28 3c 61 20 68 72 65 66 3d 22 2e 2f 69   /a>(<a href="./i
0340  6e 66 6f 2f 6d 69 64 6c 65 74 5f 6a 61 72 73 69   nfo/midlet_jarsi
0350  7a 65 2e 77 6d 6c 22 3e 69 6e 66 6f 3c 2f 61 3e   ze.wml">info</a>
0360  29 3c 62 72 2f 3e 0d 0a 09 3c 61 20 68 72 65 66   )<br/>...<a href
0370  3d 22 2e 2f 6d 69 64 6c 65 74 73 2f 4d 49 44 6c   ="./midlets/MIDl
0380  65 74 5f 43 33 2e 6a 61 64 22 3e 4d 49 44 6c 65   et_C3.jad">MIDle
0390  74 20 4e 61 6d 65 3c 2f 61 3e 28 3c 61 20 68 72   t Name</a>(<a hr
03a0  65 66 3d 22 2e 2f 69 6e 66 6f 2f 6d 69 64 6c 65   ef="./info/midle
03b0  74 5f 6e 61 6d 65 2e 77 6d 6c 22 3e 69 6e 66 6f   t_name.wml">info
03c0  3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c 61 20   </a>)<br/>...<a 
03d0  68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74 73 2f   href="./midlets/
03e0  4d 49 44 6c 65 74 5f 43 34 2e 6a 61 64 22 3e 4d   MIDlet_C4.jad">M
03f0  49 44 6c 65 74 20 56 65 72 73 69 6f 6e 3c 2f 61   IDlet Version</a
0400  3e 28 3c 61 20 68 72 65 66 3d 22 2e 2f 69 6e 66   >(<a href="./inf
0410  6f 2f 6d 69 64 6c 65 74 5f 76 65 72 73 69 6f 6e   o/midlet_version
0420  2e 77 6d 6c 22 3e 69 6e 66 6f 3c 2f 61 3e 29 3c   .wml">info</a>)<
0430  62 72 2f 3e 0d 0a 09 3c 61 20 68 72 65 66 3d 22   br/>...<a href="
0440  2e 2f 6d 69 64 6c 65 74 73 2f 4d 49 44 6c 65 74   ./midlets/MIDlet
0450  5f 43 35 2e 6a 61 64 22 3e 4d 49 44 6c 65 74 20   _C5.jad">MIDlet 
0460  56 65 6e 64 6f 72 3c 2f 61 3e 28 3c 61 20 68 72   Vendor</a>(<a hr
0470  65 66 3d 22 2e 2f 69 6e 66 6f 2f 6d 69 64 6c 65   ef="./info/midle
0480  74 5f 76 65 6e 64 6f 72 2e 77 6d 6c 22 3e 69 6e   t_vendor.wml">in
0490  66 6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c   fo</a>)<br/>...<
04a0  61 20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74   a href="./midlet
04b0  73 2f 4d 49 44 6c 65 74 5f 44 31 2e 6a 61 64 22   s/MIDlet_D1.jad"
04c0  3e 53 74 6f 70 57 61 74 63 68 3c 2f 61 3e 28 3c   >StopWatch</a>(<
04d0  61 20 68 72 65 66 3d 22 2e 2f 69 6e 66 6f 2f 73   a href="./info/s
04e0  74 6f 70 77 61 74 63 68 2e 77 6d 6c 22 3e 69 6e   topwatch.wml">in
04f0  66 6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c   fo</a>)<br/>...<
0500  61 20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74   a href="./midlet
0510  73 2f 4d 49 44 6c 65 74 5f 45 31 2e 6a 61 64 22   s/MIDlet_E1.jad"
0520  3e 4d 49 44 6c 65 74 20 76 31 2e 30 20 28 44 65   >MIDlet v1.0 (De
0530  6c 65 74 65 20 43 6f 6e 66 69 72 6d 29 3c 2f 61   lete Confirm)</a
0540  3e 28 3c 61 20 68 72 65 66 3d 22 2e 2f 69 6e 66   >(<a href="./inf
0550  6f 2f 6d 69 64 6c 65 74 5f 76 31 2e 77 6d 6c 22   o/midlet_v1.wml"
0560  3e 69 6e 66 6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d   >info</a>)<br/>.
0570  0a 09 3c 61 20 68 72 65 66 3d 22 2e 2f 6d 69 64   ..<a href="./mid
0580  6c 65 74 73 2f 4d 49 44 6c 65 74 5f 45 32 2f 4d   lets/MIDlet_E2/M
0590  49 44 6c 65 74 5f 45 31 2e 6a 61 64 22 3e 4d 49   IDlet_E1.jad">MI
05a0  44 6c 65 74 20 76 32 2e 30 3c 2f 61 3e 28 3c 61   Dlet v2.0</a>(<a
05b0  20 68 72 65 66 3d 22 2e 2f 69 6e 66 6f 2f 6d 69    href="./info/mi
05c0  64 6c 65 74 5f 76 32 2e 77 6d 6c 22 3e 69 6e 66   dlet_v2.wml">inf
05d0  6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 0d 0a   o</a>)<br/>.....
05e0  3c 2f 70 3e 0d 0a 3c 2f 63 61                     </p>..</ca

Frame 34 (65 bytes on wire, 65 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.176216000
    Time delta from previous packet: 0.000014000 seconds
    Time since reference or first frame: 14.054867000 seconds
    Frame Number: 34
    Packet Length: 65 bytes
    Capture Length: 65 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 51
    Identification: 0x7578 (30072)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2ea5)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48021 (48021), Seq: 1461, Ack: 738, Len: 11
    Source port: http (80)
    Destination port: 48021 (48021)
    Sequence number: 1461
    Next sequence number: 1472
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x56cd (incorrect, should be 0xcfbb)
Hypertext Transfer Protocol
    Data (11 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 33 75 78 40 00 80 06 00 00 c3 eb a0 50 c3 37   .3ux@........P.7
0020  2f 34 00 50 bb 95 bd 25 67 bf fc fa d4 77 50 18   /4.P...%g....wP.
0030  41 8f 56 cd 00 00 72 64 3e 0d 0a 3c 2f 77 6d 6c   A.V...rd>..</wml
0040  3e                                                >

Frame 35 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.176258000
    Time delta from previous packet: 0.000042000 seconds
    Time since reference or first frame: 14.054909000 seconds
    Frame Number: 35
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x7579 (30073)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eaf)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48021 (48021), Seq: 1472, Ack: 738, Len: 0
    Source port: http (80)
    Destination port: 48021 (48021)
    Sequence number: 1472
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16783
    Checksum: 0x56c2 (incorrect, should be 0x6554)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 79 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(uy@........P.7
0020  2f 34 00 50 bb 95 bd 25 67 ca fc fa d4 77 50 11   /4.P...%g....wP.
0030  41 8f 56 c2 00 00                                 A.V...

Frame 36 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.177075000
    Time delta from previous packet: 0.000817000 seconds
    Time since reference or first frame: 14.055726000 seconds
    Frame Number: 36
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x74b9 (29881)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x6f6f (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48021 (48021), Dst Port: http (80), Seq: 738, Ack: 1461, Len: 0
    Source port: 48021 (48021)
    Destination port: http (80)
    Sequence number: 738
    Acknowledgement number: 1461
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 7300
    Checksum: 0x8a6b (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 33
        The RTT to ACK the segment was: 0.000873000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 74 b9 40 00 40 06 6f 6f c3 37 2f 34 c3 eb   .(t.@.@.oo.7/4..
0020  a0 50 bb 95 00 50 fc fa d4 77 bd 25 67 bf 50 10   .P...P...w.%g.P.
0030  1c 84 8a 6b 00 00 00 00 00 00 00 00               ...k........

Frame 37 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.193125000
    Time delta from previous packet: 0.016050000 seconds
    Time since reference or first frame: 14.071776000 seconds
    Frame Number: 37
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x74ba (29882)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0x6f6e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48021 (48021), Dst Port: http (80), Seq: 738, Ack: 1473, Len: 0
    Source port: 48021 (48021)
    Destination port: http (80)
    Sequence number: 738
    Acknowledgement number: 1473
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 7300
    Checksum: 0x8a5e (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 35
        The RTT to ACK the segment was: 0.016867000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 74 ba 40 00 40 06 6f 6e c3 37 2f 34 c3 eb   .(t.@.@.on.7/4..
0020  a0 50 bb 95 00 50 fc fa d4 77 bd 25 67 cb 50 11   .P...P...w.%g.P.
0030  1c 84 8a 5e 00 00 00 00 00 00 00 00               ...^........

Frame 38 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:28.193133000
    Time delta from previous packet: 0.000008000 seconds
    Time since reference or first frame: 14.071784000 seconds
    Frame Number: 38
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x757a (30074)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eae)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48021 (48021), Seq: 1473, Ack: 739, Len: 0
    Source port: http (80)
    Destination port: 48021 (48021)
    Sequence number: 1473
    Acknowledgement number: 739
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x56c2 (incorrect, should be 0x6553)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 37
        The RTT to ACK the segment was: 0.000008000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 7a 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(uz@........P.7
0020  2f 34 00 50 bb 95 bd 25 67 cb fc fa d4 78 50 10   /4.P...%g....xP.
0030  41 8f 56 c2 00 00                                 A.V...

Frame 39 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.742931000
    Time delta from previous packet: 3.549798000 seconds
    Time since reference or first frame: 17.621582000 seconds
    Frame Number: 39
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0xeff1 (61425)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0xf7ce (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0x7479 (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 ef f1 40 00 3c 06 f7 ce c3 37 2f 34 c3 eb   .0..@.<....7/4..
0020  a0 50 bc 1c 00 50 42 79 58 24 00 00 00 00 70 02   .P...PByX$....p.
0030  60 f4 74 79 00 00 02 04 05 b4 01 01 04 02         `.ty..........

Frame 40 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.742965000
    Time delta from previous packet: 0.000034000 seconds
    Time since reference or first frame: 17.621616000 seconds
    Frame Number: 40
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x757b (30075)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2ea5)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48156 (48156), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 48156 (48156)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0x121f (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 39
        The RTT to ACK the segment was: 0.000034000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 7b 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0u{@........P.7
0020  2f 34 00 50 bc 1c 27 5b 57 72 42 79 58 25 70 12   /4.P..'[WrByX%p.
0030  44 70 12 1f 00 00 02 04 05 b4 01 01 04 02         Dp............

Frame 41 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.794969000
    Time delta from previous packet: 0.052004000 seconds
    Time since reference or first frame: 17.673620000 seconds
    Frame Number: 41
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x0959 (2393)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xdacf (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x6de3 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 40
        The RTT to ACK the segment was: 0.052004000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 09 59 40 00 40 06 da cf c3 37 2f 34 c3 eb   .(.Y@.@....7/4..
0020  a0 50 bc 1c 00 50 42 79 58 25 27 5b 57 73 50 10   .P...PByX%'[WsP.
0030  15 70 6d e3 00 00 00 00 00 00 00 00               .pm.........

Frame 42 (787 bytes on wire, 787 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.824642000
    Time delta from previous packet: 0.029673000 seconds
    Time since reference or first frame: 17.703293000 seconds
    Frame Number: 42
    Packet Length: 787 bytes
    Capture Length: 787 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 773
    Identification: 0x095a (2394)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xd7f1 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 1, Ack: 1, Len: 733
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 734
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x5792 (correct)
Hypertext Transfer Protocol
    GET /java/midp10/midlets/MIDlet_C1.jad HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/java/midp10/index_midp1.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  03 05 09 5a 40 00 40 06 d7 f1 c3 37 2f 34 c3 eb   ...Z@.@....7/4..
0020  a0 50 bc 1c 00 50 42 79 58 25 27 5b 57 73 50 18   .P...PByX%'[WsP.
0030  15 70 57 92 00 00 47 45 54 20 2f 6a 61 76 61 2f   .pW...GET /java/
0040  6d 69 64 70 31 30 2f 6d 69 64 6c 65 74 73 2f 4d   midp10/midlets/M
0050  49 44 6c 65 74 5f 43 31 2e 6a 61 64 20 48 54 54   IDlet_C1.jad HTT
0060  50 2f 31 2e 31 0d 0a 54 4d 5f 75 73 65 72 2d 69   P/1.1..TM_user-i
0070  64 3a 20 30 33 34 36 30 32 37 33 38 34 33 31 35   d: 0346027384315
0080  34 36 31 33 30 37 0d 0a 78 2d 75 70 2d 73 75 62   461307..x-up-sub
0090  6e 6f 3a 20 30 33 34 36 30 32 37 33 38 34 33 31   no: 034602738431
00a0  35 34 36 31 33 30 37 0d 0a 48 6f 73 74 3a 20 31   5461307..Host: 1
00b0  39 35 2e 32 33 35 2e 31 36 30 2e 38 30 0d 0a 41   95.235.160.80..A
00c0  63 63 65 70 74 3a 20 6d 75 6c 74 69 70 61 72 74   ccept: multipart
00d0  2f 6d 69 78 65 64 2c 20 61 70 70 6c 69 63 61 74   /mixed, applicat
00e0  69 6f 6e 2f 76 6e 64 2e 77 61 70 2e 6d 75 6c 74   ion/vnd.wap.mult
00f0  69 70 61 72 74 2e 6d 69 78 65 64 2c 20 61 70 70   ipart.mixed, app
0100  6c 69 63 61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70   lication/vnd.wap
0110  2e 78 68 74 6d 6c 2b 78 6d 6c 2c 20 61 70 70 6c   .xhtml+xml, appl
0120  69 63 61 74 69 6f 6e 2f 78 68 74 6d 6c 2b 78 6d   ication/xhtml+xm
0130  6c 2c 20 74 65 78 74 2f 76 6e 64 2e 77 61 70 2e   l, text/vnd.wap.
0140  77 6d 6c 2c 20 2a 2f 2a 2c 2a 2f 2a 0d 0a 41 63   wml, */*,*/*..Ac
0150  63 65 70 74 2d 43 68 61 72 73 65 74 3a 20 75 74   cept-Charset: ut
0160  66 2d 38 2c 20 75 74 66 2d 31 36 2c 20 69 73 6f   f-8, utf-16, iso
0170  2d 38 38 35 39 2d 31 2c 20 69 73 6f 2d 31 30 36   -8859-1, iso-106
0180  34 36 2d 75 63 73 2d 32 2c 20 53 68 69 66 74 5f   46-ucs-2, Shift_
0190  4a 49 53 2c 20 42 69 67 35 2c 2a 0d 0a 41 63 63   JIS, Big5,*..Acc
01a0  65 70 74 2d 45 6e 63 6f 64 69 6e 67 3a 20 67 7a   ept-Encoding: gz
01b0  69 70 2c 20 64 65 66 6c 61 74 65 0d 0a 41 63 63   ip, deflate..Acc
01c0  65 70 74 2d 4c 61 6e 67 75 61 67 65 3a 20 65 73   ept-Language: es
01d0  0d 0a 52 65 66 65 72 65 72 3a 20 68 74 74 70 3a   ..Referer: http:
01e0  2f 2f 31 39 35 2e 32 33 35 2e 31 36 30 2e 38 30   //195.235.160.80
01f0  2f 6a 61 76 61 2f 6d 69 64 70 31 30 2f 69 6e 64   /java/midp10/ind
0200  65 78 5f 6d 69 64 70 31 2e 77 6d 6c 0d 0a 55 73   ex_midp1.wml..Us
0210  65 72 2d 41 67 65 6e 74 3a 20 53 6f 6e 79 45 72   er-Agent: SonyEr
0220  69 63 73 73 6f 6e 5a 35 33 30 69 2f 52 36 41 43   icssonZ530i/R6AC
0230  20 42 72 6f 77 73 65 72 2f 4e 65 74 46 72 6f 6e    Browser/NetFron
0240  74 2f 33 2e 33 20 50 72 6f 66 69 6c 65 2f 4d 49   t/3.3 Profile/MI
0250  44 50 2d 32 2e 30 20 43 6f 6e 66 69 67 75 72 61   DP-2.0 Configura
0260  74 69 6f 6e 2f 43 4c 44 43 2d 31 2e 31 20 55 50   tion/CLDC-1.1 UP
0270  2e 4c 69 6e 6b 2f 36 2e 32 2e 33 2e 31 35 2e 30   .Link/6.2.3.15.0
0280  0d 0a 78 2d 77 61 70 2d 70 72 6f 66 69 6c 65 3a   ..x-wap-profile:
0290  20 22 68 74 74 70 3a 2f 2f 77 61 70 2e 73 6f 6e    "http://wap.son
02a0  79 65 72 69 63 73 73 6f 6e 2e 63 6f 6d 2f 55 41   yericsson.com/UA
02b0  70 72 6f 66 2f 5a 35 33 30 69 52 32 30 31 2e 78   prof/Z530iR201.x
02c0  6d 6c 22 0d 0a 78 2d 75 70 2d 66 6f 72 77 61 72   ml"..x-up-forwar
02d0  64 65 64 2d 66 6f 72 3a 20 31 30 2e 31 34 36 2e   ded-for: 10.146.
02e0  36 33 2e 30 0d 0a 56 69 61 3a 20 31 2e 31 20 6d   63.0..Via: 1.1 m
02f0  62 65 2d 70 72 6f 78 79 32 70 65 2e 77 61 70 2e   be-proxy2pe.wap.
0300  6f 6c 65 61 64 61 2e 63 6f 6d 3a 38 30 38 30 0d   oleada.com:8080.
0310  0a 0d 0a                                          ...

Frame 43 (705 bytes on wire, 705 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.825578000
    Time delta from previous packet: 0.000936000 seconds
    Time since reference or first frame: 17.704229000 seconds
    Frame Number: 43
    Packet Length: 705 bytes
    Capture Length: 705 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 691
    Identification: 0x757c (30076)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2c21)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48156 (48156), Seq: 1, Ack: 734, Len: 651
    Source port: http (80)
    Destination port: 48156 (48156)
    Sequence number: 1
    Next sequence number: 652
    Acknowledgement number: 734
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16787
    Checksum: 0x594d (incorrect, should be 0x5fb6)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 42
        The RTT to ACK the segment was: 0.000936000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:31 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Thu, 30 Sep 2004 13:35:16 GMT\r\n
    ETag: "0-193-415c0b94"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 403\r\n
    Content-Type: text/vnd.sun.j2me.app-descriptor\r\n
    \r\n
    MIDlet-1: MIDlet_C1, MIDlet_C1.png, WirelessMIDlet\r\n
    MIDlet-Description: Developed by Manuel Perez\r\n
    MIDlet-Install-Notify: http://195.235.160.80:8080/servlet/InstallNotify\r\n
    MIDlet-Jar-Size: 4786\r\n
    MIDlet-Jar-URL: http://195.235.160.80/java/midp10/midlets/MIDlet_C1.jar\r\n
    MIDlet-Name: MIDlet_C1\r\n
    MIDlet-Vendor: TME\r\n
    MIDlet-Version: 1.0\r\n
    MicroEdition-Configuration: CLDC-1.0\r\n
    MicroEdition-Profile: MIDP-1.0\r\n

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  02 b3 75 7c 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..u|@........P.7
0020  2f 34 00 50 bc 1c 27 5b 57 73 42 79 5b 02 50 18   /4.P..'[WsBy[.P.
0030  41 93 59 4d 00 00 48 54 54 50 2f 31 2e 31 20 32   A.YM..HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 33 31 20 47 4d 54 0d 0a 53 65 72 76   :42:31 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 54 68 75 2c 20 33   Modified: Thu, 3
00a0  30 20 53 65 70 20 32 30 30 34 20 31 33 3a 33 35   0 Sep 2004 13:35
00b0  3a 31 36 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :16 GMT..ETag: "
00c0  30 2d 31 39 33 2d 34 31 35 63 30 62 39 34 22 0d   0-193-415c0b94".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 34 30 33 0d 0a 43 6f 6e 74   ength: 403..Cont
0100  65 6e 74 2d 54 79 70 65 3a 20 74 65 78 74 2f 76   ent-Type: text/v
0110  6e 64 2e 73 75 6e 2e 6a 32 6d 65 2e 61 70 70 2d   nd.sun.j2me.app-
0120  64 65 73 63 72 69 70 74 6f 72 0d 0a 0d 0a 4d 49   descriptor....MI
0130  44 6c 65 74 2d 31 3a 20 4d 49 44 6c 65 74 5f 43   Dlet-1: MIDlet_C
0140  31 2c 20 4d 49 44 6c 65 74 5f 43 31 2e 70 6e 67   1, MIDlet_C1.png
0150  2c 20 57 69 72 65 6c 65 73 73 4d 49 44 6c 65 74   , WirelessMIDlet
0160  0d 0a 4d 49 44 6c 65 74 2d 44 65 73 63 72 69 70   ..MIDlet-Descrip
0170  74 69 6f 6e 3a 20 44 65 76 65 6c 6f 70 65 64 20   tion: Developed 
0180  62 79 20 4d 61 6e 75 65 6c 20 50 65 72 65 7a 0d   by Manuel Perez.
0190  0a 4d 49 44 6c 65 74 2d 49 6e 73 74 61 6c 6c 2d   .MIDlet-Install-
01a0  4e 6f 74 69 66 79 3a 20 68 74 74 70 3a 2f 2f 31   Notify: http://1
01b0  39 35 2e 32 33 35 2e 31 36 30 2e 38 30 3a 38 30   95.235.160.80:80
01c0  38 30 2f 73 65 72 76 6c 65 74 2f 49 6e 73 74 61   80/servlet/Insta
01d0  6c 6c 4e 6f 74 69 66 79 0d 0a 4d 49 44 6c 65 74   llNotify..MIDlet
01e0  2d 4a 61 72 2d 53 69 7a 65 3a 20 34 37 38 36 0d   -Jar-Size: 4786.
01f0  0a 4d 49 44 6c 65 74 2d 4a 61 72 2d 55 52 4c 3a   .MIDlet-Jar-URL:
0200  20 68 74 74 70 3a 2f 2f 31 39 35 2e 32 33 35 2e    http://195.235.
0210  31 36 30 2e 38 30 2f 6a 61 76 61 2f 6d 69 64 70   160.80/java/midp
0220  31 30 2f 6d 69 64 6c 65 74 73 2f 4d 49 44 6c 65   10/midlets/MIDle
0230  74 5f 43 31 2e 6a 61 72 0d 0a 4d 49 44 6c 65 74   t_C1.jar..MIDlet
0240  2d 4e 61 6d 65 3a 20 4d 49 44 6c 65 74 5f 43 31   -Name: MIDlet_C1
0250  0d 0a 4d 49 44 6c 65 74 2d 56 65 6e 64 6f 72 3a   ..MIDlet-Vendor:
0260  20 54 4d 45 0d 0a 4d 49 44 6c 65 74 2d 56 65 72    TME..MIDlet-Ver
0270  73 69 6f 6e 3a 20 31 2e 30 0d 0a 4d 69 63 72 6f   sion: 1.0..Micro
0280  45 64 69 74 69 6f 6e 2d 43 6f 6e 66 69 67 75 72   Edition-Configur
0290  61 74 69 6f 6e 3a 20 43 4c 44 43 2d 31 2e 30 0d   ation: CLDC-1.0.
02a0  0a 4d 69 63 72 6f 45 64 69 74 69 6f 6e 2d 50 72   .MicroEdition-Pr
02b0  6f 66 69 6c 65 3a 20 4d 49 44 50 2d 31 2e 30 0d   ofile: MIDP-1.0.
02c0  0a                                                .

Frame 44 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:31.826341000
    Time delta from previous packet: 0.000763000 seconds
    Time since reference or first frame: 17.704992000 seconds
    Frame Number: 44
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x095b (2395)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xdacd (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 734, Ack: 652, Len: 0
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 734
    Acknowledgement number: 652
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6510
    Checksum: 0x647d (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 43
        The RTT to ACK the segment was: 0.000763000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 09 5b 40 00 40 06 da cd c3 37 2f 34 c3 eb   .(.[@.@....7/4..
0020  a0 50 bc 1c 00 50 42 79 5b 02 27 5b 59 fe 50 10   .P...PBy[.'[Y.P.
0030  19 6e 64 7d 00 00 00 00 00 00 00 00               .nd}........

Frame 45 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:32.643701000
    Time delta from previous packet: 0.817360000 seconds
    Time since reference or first frame: 18.522352000 seconds
    Frame Number: 45
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x095c (2396)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xdacc (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 734, Ack: 652, Len: 0
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 734
    Acknowledgement number: 652
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 6510
    Checksum: 0x647c (correct)

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 09 5c 40 00 40 06 da cc c3 37 2f 34 c3 eb   .(.\@.@....7/4..
0020  a0 50 bc 1c 00 50 42 79 5b 02 27 5b 59 fe 50 11   .P...PBy[.'[Y.P.
0030  19 6e 64 7c 00 00 00 00 00 00 00 00               .nd|........

Frame 46 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:32.643737000
    Time delta from previous packet: 0.000036000 seconds
    Time since reference or first frame: 18.522388000 seconds
    Frame Number: 46
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x757d (30077)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eab)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48156 (48156), Seq: 652, Ack: 735, Len: 0
    Source port: http (80)
    Destination port: 48156 (48156)
    Sequence number: 652
    Acknowledgement number: 735
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16787
    Checksum: 0x56c2 (incorrect, should be 0x3c57)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 45
        The RTT to ACK the segment was: 0.000036000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 7d 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(u}@........P.7
0020  2f 34 00 50 bc 1c 27 5b 59 fe 42 79 5b 03 50 10   /4.P..'[Y.By[.P.
0030  41 93 56 c2 00 00                                 A.V...

Frame 47 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:32.643807000
    Time delta from previous packet: 0.000070000 seconds
    Time since reference or first frame: 18.522458000 seconds
    Frame Number: 47
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x757e (30078)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2eaa)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48156 (48156), Seq: 652, Ack: 735, Len: 0
    Source port: http (80)
    Destination port: 48156 (48156)
    Sequence number: 652
    Acknowledgement number: 735
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16787
    Checksum: 0x56c2 (incorrect, should be 0x3c56)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 7e 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(u~@........P.7
0020  2f 34 00 50 bc 1c 27 5b 59 fe 42 79 5b 03 50 11   /4.P..'[Y.By[.P.
0030  41 93 56 c2 00 00                                 A.V...

Frame 48 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:32.644179000
    Time delta from previous packet: 0.000372000 seconds
    Time since reference or first frame: 18.522830000 seconds
    Frame Number: 48
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0xe720 (59168)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xfd07 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48156 (48156), Dst Port: http (80), Seq: 735, Ack: 653, Len: 0
    Source port: 48156 (48156)
    Destination port: http (80)
    Sequence number: 735
    Acknowledgement number: 653
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 6510
    Checksum: 0x647b (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 47
        The RTT to ACK the segment was: 0.000372000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 e7 20 40 00 40 06 fd 07 c3 37 2f 34 c3 eb   .(. @.@....7/4..
0020  a0 50 bc 1c 00 50 42 79 5b 03 27 5b 59 ff 50 10   .P...PBy[.'[Y.P.
0030  19 6e 64 7b 00 00 00 00 00 00 00 00               .nd{........

Frame 49 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.464727000
    Time delta from previous packet: 15.820548000 seconds
    Time since reference or first frame: 34.343378000 seconds
    Frame Number: 49
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x60 (DSCP 0x18: Class Selector 3; ECN: 0x00)
        0110 00.. = Differentiated Services Codepoint: Class Selector 3 (0x18)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7c92 (31890)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 60
    Protocol: TCP (0x06)
    Header checksum: 0x6b2e (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48832 (48832), Dst Port: http (80), Seq: 0, Ack: 0, Len: 0
    Source port: 48832 (48832)
    Destination port: http (80)
    Sequence number: 0
    Header length: 28 bytes
    Flags: 0x0002 (SYN)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...0 .... = Acknowledgment: Not set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 24820
    Checksum: 0xffea (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 60   ..V..|.. ..Q..E`
0010  00 30 7c 92 40 00 3c 06 6b 2e c3 37 2f 34 c3 eb   .0|.@.<.k..7/4..
0020  a0 50 be c0 00 50 53 96 b8 f1 00 00 00 00 70 02   .P...PS.......p.
0030  60 f4 ff ea 00 00 02 04 05 b4 01 01 04 02         `.............

Frame 50 (62 bytes on wire, 62 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.464762000
    Time delta from previous packet: 0.000035000 seconds
    Time since reference or first frame: 34.343413000 seconds
    Frame Number: 50
    Packet Length: 62 bytes
    Capture Length: 62 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 48
    Identification: 0x7587 (30087)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2e99)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48832 (48832), Seq: 0, Ack: 1, Len: 0
    Source port: http (80)
    Destination port: 48832 (48832)
    Sequence number: 0
    Acknowledgement number: 1
    Header length: 28 bytes
    Flags: 0x0012 (SYN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..1. = Syn: Set
        .... ...0 = Fin: Not set
    Window size: 17520
    Checksum: 0xd3fa (correct)
    Options: (8 bytes)
        Maximum segment size: 1460 bytes
        NOP
        NOP
        SACK permitted
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 49
        The RTT to ACK the segment was: 0.000035000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 30 75 87 40 00 80 06 00 00 c3 eb a0 50 c3 37   .0u.@........P.7
0020  2f 34 00 50 be c0 7b 55 cd 0d 53 96 b8 f2 70 12   /4.P..{U..S...p.
0030  44 70 d3 fa 00 00 02 04 05 b4 01 01 04 02         Dp............

Frame 51 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.516034000
    Time delta from previous packet: 0.051272000 seconds
    Time since reference or first frame: 34.394685000 seconds
    Frame Number: 51
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x32cc (13004)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xb15c (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48832 (48832), Dst Port: http (80), Seq: 1, Ack: 1, Len: 0
    Source port: 48832 (48832)
    Destination port: http (80)
    Sequence number: 1
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0x2fbf (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 50
        The RTT to ACK the segment was: 0.051272000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 32 cc 40 00 40 06 b1 5c c3 37 2f 34 c3 eb   .(2.@.@..\.7/4..
0020  a0 50 be c0 00 50 53 96 b8 f2 7b 55 cd 0e 50 10   .P...PS...{U..P.
0030  15 70 2f bf 00 00 00 00 00 00 00 00               .p/.........

Frame 52 (791 bytes on wire, 791 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.518710000
    Time delta from previous packet: 0.002676000 seconds
    Time since reference or first frame: 34.397361000 seconds
    Frame Number: 52
    Packet Length: 791 bytes
    Capture Length: 791 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 777
    Identification: 0x32cd (13005)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xae7a (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48832 (48832), Dst Port: http (80), Seq: 1, Ack: 1, Len: 737
    Source port: 48832 (48832)
    Destination port: http (80)
    Sequence number: 1
    Next sequence number: 738
    Acknowledgement number: 1
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 5488
    Checksum: 0xa1b5 (correct)
Hypertext Transfer Protocol
    GET /java/midp20/index_midp2.wml HTTP/1.1\r\n
        Request Method: GET
    TM_user-id: 0346027384315461307\r\n
    x-up-subno: 0346027384315461307\r\n
    Connection: close\r\n
    Host: 195.235.160.80\r\n
    Accept: multipart/mixed, application/vnd.wap.multipart.mixed, application/vnd.wap.xhtml+xml, application/xhtml+xml, text/vnd.wap.wml, */*,*/*\r\n
    Accept-Charset: utf-8, utf-16, iso-8859-1, iso-10646-ucs-2, Shift_JIS, Big5,*\r\n
    Accept-Encoding: gzip, deflate\r\n
    Accept-Language: es\r\n
    Referer: http://195.235.160.80/java/index_tme.wml\r\n
    User-Agent: SonyEricssonZ530i/R6AC Browser/NetFront/3.3 Profile/MIDP-2.0 Configuration/CLDC-1.1 UP.Link/6.2.3.15.0\r\n
    x-wap-profile: "http://wap.sonyericsson.com/UAprof/Z530iR201.xml"\r\n
    x-up-forwarded-for: 10.146.63.0\r\n
    Via: 1.1 mbe-proxy2pe.wap.oleada.com:8080\r\n
    \r\n

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  03 09 32 cd 40 00 40 06 ae 7a c3 37 2f 34 c3 eb   ..2.@.@..z.7/4..
0020  a0 50 be c0 00 50 53 96 b8 f2 7b 55 cd 0e 50 18   .P...PS...{U..P.
0030  15 70 a1 b5 00 00 47 45 54 20 2f 6a 61 76 61 2f   .p....GET /java/
0040  6d 69 64 70 32 30 2f 69 6e 64 65 78 5f 6d 69 64   midp20/index_mid
0050  70 32 2e 77 6d 6c 20 48 54 54 50 2f 31 2e 31 0d   p2.wml HTTP/1.1.
0060  0a 54 4d 5f 75 73 65 72 2d 69 64 3a 20 30 33 34   .TM_user-id: 034
0070  36 30 32 37 33 38 34 33 31 35 34 36 31 33 30 37   6027384315461307
0080  0d 0a 78 2d 75 70 2d 73 75 62 6e 6f 3a 20 30 33   ..x-up-subno: 03
0090  34 36 30 32 37 33 38 34 33 31 35 34 36 31 33 30   4602738431546130
00a0  37 0d 0a 43 6f 6e 6e 65 63 74 69 6f 6e 3a 20 63   7..Connection: c
00b0  6c 6f 73 65 0d 0a 48 6f 73 74 3a 20 31 39 35 2e   lose..Host: 195.
00c0  32 33 35 2e 31 36 30 2e 38 30 0d 0a 41 63 63 65   235.160.80..Acce
00d0  70 74 3a 20 6d 75 6c 74 69 70 61 72 74 2f 6d 69   pt: multipart/mi
00e0  78 65 64 2c 20 61 70 70 6c 69 63 61 74 69 6f 6e   xed, application
00f0  2f 76 6e 64 2e 77 61 70 2e 6d 75 6c 74 69 70 61   /vnd.wap.multipa
0100  72 74 2e 6d 69 78 65 64 2c 20 61 70 70 6c 69 63   rt.mixed, applic
0110  61 74 69 6f 6e 2f 76 6e 64 2e 77 61 70 2e 78 68   ation/vnd.wap.xh
0120  74 6d 6c 2b 78 6d 6c 2c 20 61 70 70 6c 69 63 61   tml+xml, applica
0130  74 69 6f 6e 2f 78 68 74 6d 6c 2b 78 6d 6c 2c 20   tion/xhtml+xml, 
0140  74 65 78 74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c   text/vnd.wap.wml
0150  2c 20 2a 2f 2a 2c 2a 2f 2a 0d 0a 41 63 63 65 70   , */*,*/*..Accep
0160  74 2d 43 68 61 72 73 65 74 3a 20 75 74 66 2d 38   t-Charset: utf-8
0170  2c 20 75 74 66 2d 31 36 2c 20 69 73 6f 2d 38 38   , utf-16, iso-88
0180  35 39 2d 31 2c 20 69 73 6f 2d 31 30 36 34 36 2d   59-1, iso-10646-
0190  75 63 73 2d 32 2c 20 53 68 69 66 74 5f 4a 49 53   ucs-2, Shift_JIS
01a0  2c 20 42 69 67 35 2c 2a 0d 0a 41 63 63 65 70 74   , Big5,*..Accept
01b0  2d 45 6e 63 6f 64 69 6e 67 3a 20 67 7a 69 70 2c   -Encoding: gzip,
01c0  20 64 65 66 6c 61 74 65 0d 0a 41 63 63 65 70 74    deflate..Accept
01d0  2d 4c 61 6e 67 75 61 67 65 3a 20 65 73 0d 0a 52   -Language: es..R
01e0  65 66 65 72 65 72 3a 20 68 74 74 70 3a 2f 2f 31   eferer: http://1
01f0  39 35 2e 32 33 35 2e 31 36 30 2e 38 30 2f 6a 61   95.235.160.80/ja
0200  76 61 2f 69 6e 64 65 78 5f 74 6d 65 2e 77 6d 6c   va/index_tme.wml
0210  0d 0a 55 73 65 72 2d 41 67 65 6e 74 3a 20 53 6f   ..User-Agent: So
0220  6e 79 45 72 69 63 73 73 6f 6e 5a 35 33 30 69 2f   nyEricssonZ530i/
0230  52 36 41 43 20 42 72 6f 77 73 65 72 2f 4e 65 74   R6AC Browser/Net
0240  46 72 6f 6e 74 2f 33 2e 33 20 50 72 6f 66 69 6c   Front/3.3 Profil
0250  65 2f 4d 49 44 50 2d 32 2e 30 20 43 6f 6e 66 69   e/MIDP-2.0 Confi
0260  67 75 72 61 74 69 6f 6e 2f 43 4c 44 43 2d 31 2e   guration/CLDC-1.
0270  31 20 55 50 2e 4c 69 6e 6b 2f 36 2e 32 2e 33 2e   1 UP.Link/6.2.3.
0280  31 35 2e 30 0d 0a 78 2d 77 61 70 2d 70 72 6f 66   15.0..x-wap-prof
0290  69 6c 65 3a 20 22 68 74 74 70 3a 2f 2f 77 61 70   ile: "http://wap
02a0  2e 73 6f 6e 79 65 72 69 63 73 73 6f 6e 2e 63 6f   .sonyericsson.co
02b0  6d 2f 55 41 70 72 6f 66 2f 5a 35 33 30 69 52 32   m/UAprof/Z530iR2
02c0  30 31 2e 78 6d 6c 22 0d 0a 78 2d 75 70 2d 66 6f   01.xml"..x-up-fo
02d0  72 77 61 72 64 65 64 2d 66 6f 72 3a 20 31 30 2e   rwarded-for: 10.
02e0  31 34 36 2e 36 33 2e 30 0d 0a 56 69 61 3a 20 31   146.63.0..Via: 1
02f0  2e 31 20 6d 62 65 2d 70 72 6f 78 79 32 70 65 2e   .1 mbe-proxy2pe.
0300  77 61 70 2e 6f 6c 65 61 64 61 2e 63 6f 6d 3a 38   wap.oleada.com:8
0310  30 38 30 0d 0a 0d 0a                              080....

Frame 53 (1514 bytes on wire, 1514 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.519677000
    Time delta from previous packet: 0.000967000 seconds
    Time since reference or first frame: 34.398328000 seconds
    Frame Number: 53
    Packet Length: 1514 bytes
    Capture Length: 1514 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 1500
    Identification: 0x7588 (30088)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x28ec)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48832 (48832), Seq: 1, Ack: 738, Len: 1460
    Source port: http (80)
    Destination port: 48832 (48832)
    Sequence number: 1
    Next sequence number: 1461
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x5c76 (incorrect, should be 0xfd1e)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 52
        The RTT to ACK the segment was: 0.000967000 seconds
Hypertext Transfer Protocol
    HTTP/1.1 200 OK\r\n
        Response Code: 200
    Date: Wed, 26 Apr 2006 10:42:48 GMT\r\n
    Server: Apache/1.3.29 (Win32)\r\n
    Last-Modified: Tue, 15 Nov 2005 17:37:23 GMT\r\n
    ETag: "0-56f-437a1cd3"\r\n
    Accept-Ranges: bytes\r\n
    Content-Length: 1391\r\n
    Connection: close\r\n
    Content-Type: text/vnd.wap.wml\r\n
    \r\n
    Data (1208 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  05 dc 75 88 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..u.@........P.7
0020  2f 34 00 50 be c0 7b 55 cd 0e 53 96 bb d3 50 10   /4.P..{U..S...P.
0030  41 8f 5c 76 00 00 48 54 54 50 2f 31 2e 31 20 32   A.\v..HTTP/1.1 2
0040  30 30 20 4f 4b 0d 0a 44 61 74 65 3a 20 57 65 64   00 OK..Date: Wed
0050  2c 20 32 36 20 41 70 72 20 32 30 30 36 20 31 30   , 26 Apr 2006 10
0060  3a 34 32 3a 34 38 20 47 4d 54 0d 0a 53 65 72 76   :42:48 GMT..Serv
0070  65 72 3a 20 41 70 61 63 68 65 2f 31 2e 33 2e 32   er: Apache/1.3.2
0080  39 20 28 57 69 6e 33 32 29 0d 0a 4c 61 73 74 2d   9 (Win32)..Last-
0090  4d 6f 64 69 66 69 65 64 3a 20 54 75 65 2c 20 31   Modified: Tue, 1
00a0  35 20 4e 6f 76 20 32 30 30 35 20 31 37 3a 33 37   5 Nov 2005 17:37
00b0  3a 32 33 20 47 4d 54 0d 0a 45 54 61 67 3a 20 22   :23 GMT..ETag: "
00c0  30 2d 35 36 66 2d 34 33 37 61 31 63 64 33 22 0d   0-56f-437a1cd3".
00d0  0a 41 63 63 65 70 74 2d 52 61 6e 67 65 73 3a 20   .Accept-Ranges: 
00e0  62 79 74 65 73 0d 0a 43 6f 6e 74 65 6e 74 2d 4c   bytes..Content-L
00f0  65 6e 67 74 68 3a 20 31 33 39 31 0d 0a 43 6f 6e   ength: 1391..Con
0100  6e 65 63 74 69 6f 6e 3a 20 63 6c 6f 73 65 0d 0a   nection: close..
0110  43 6f 6e 74 65 6e 74 2d 54 79 70 65 3a 20 74 65   Content-Type: te
0120  78 74 2f 76 6e 64 2e 77 61 70 2e 77 6d 6c 0d 0a   xt/vnd.wap.wml..
0130  0d 0a 3c 3f 78 6d 6c 20 76 65 72 73 69 6f 6e 3d   ..<?xml version=
0140  22 31 2e 30 22 3f 3e 20 0d 0a 3c 21 44 4f 43 54   "1.0"?> ..<!DOCT
0150  59 50 45 20 77 6d 6c 20 50 55 42 4c 49 43 20 22   YPE wml PUBLIC "
0160  2d 2f 2f 57 41 50 46 4f 52 55 4d 2f 2f 44 54 44   -//WAPFORUM//DTD
0170  20 57 4d 4c 20 31 2e 31 2f 2f 45 4e 22 20 22 68    WML 1.1//EN" "h
0180  74 74 70 3a 2f 2f 77 77 77 2e 77 61 70 66 6f 72   ttp://www.wapfor
0190  75 6d 2e 6f 72 67 2f 44 54 44 2f 77 6d 6c 5f 31   um.org/DTD/wml_1
01a0  2e 31 2e 78 6d 6c 22 3e 20 0d 0a 3c 77 6d 6c 3e   .1.xml"> ..<wml>
01b0  0d 0a 3c 68 65 61 64 3e 20 0d 0a 3c 6d 65 74 61   ..<head> ..<meta
01c0  20 68 74 74 70 2d 65 71 75 69 76 3d 22 43 6f 6e    http-equiv="Con
01d0  74 65 6e 74 2d 54 79 70 65 22 20 63 6f 6e 74 65   tent-Type" conte
01e0  6e 74 3d 22 74 65 78 74 2f 76 6e 64 2e 77 61 70   nt="text/vnd.wap
01f0  2e 77 6d 6c 3b 20 63 68 61 72 73 65 74 3d 69 73   .wml; charset=is
0200  6f 2d 38 38 35 39 2d 31 22 2f 3e 0d 0a 3c 2f 68   o-8859-1"/>..</h
0210  65 61 64 3e 0d 0a 3c 63 61 72 64 20 74 69 74 6c   ead>..<card titl
0220  65 3d 22 4d 49 44 50 20 32 2e 30 20 54 65 73 74   e="MIDP 2.0 Test
0230  22 3e 0d 0a 0d 0a 3c 70 20 61 6c 69 67 6e 3d 22   ">....<p align="
0240  6c 65 66 74 22 3e 0d 0a 54 68 69 73 20 73 69 74   left">..This sit
0250  65 20 73 68 6f 77 73 20 61 20 6c 69 73 74 20 77   e shows a list w
0260  69 74 68 20 74 68 65 20 4d 49 44 6c 65 74 73 20   ith the MIDlets 
0270  75 73 65 64 20 74 6f 20 63 68 65 63 6b 20 74 68   used to check th
0280  65 20 4a 32 4d 45 20 63 6c 69 65 6e 74 20 77 69   e J2ME client wi
0290  74 68 20 74 68 65 20 4d 49 44 50 20 32 2e 30 20   th the MIDP 2.0 
02a0  64 65 76 69 63 65 73 2e 3c 62 72 2f 3e 0d 0a 0d   devices.<br/>...
02b0  0a 0d 0a 3c 21 2d 2d 0d 0a 3c 61 20 68 72 65 66   ...<!--..<a href
02c0  3d 22 2e 2f 6d 69 64 6c 65 74 73 2f 4d 49 44 6c   ="./midlets/MIDl
02d0  65 74 53 69 67 6e 65 64 2e 6a 61 64 22 3e 31 2e   etSigned.jad">1.
02e0  2d 20 4d 49 44 6c 65 74 20 73 69 67 6e 65 64 20   - MIDlet signed 
02f0  77 69 74 68 20 54 4d 45 20 63 65 72 74 69 66 69   with TME certifi
0300  63 61 74 65 3c 2f 61 3e 3c 62 72 2f 3e 0d 0a 3c   cate</a><br/>..<
0310  61 20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74   a href="./midlet
0320  73 2f 50 6c 61 74 66 6f 72 6d 52 65 71 75 65 73   s/PlatformReques
0330  74 2e 6a 61 64 22 3e 32 2e 2d 20 4d 49 44 6c 65   t.jad">2.- MIDle
0340  74 20 50 6c 61 74 66 6f 72 6d 20 52 65 71 75 65   t Platform Reque
0350  73 74 28 69 6e 69 74 69 61 74 65 3a 20 62 72 6f   st(initiate: bro
0360  77 73 65 72 20 73 65 73 73 69 6f 6e 2c 20 70 68   wser session, ph
0370  6f 6e 65 20 63 61 6c 6c 2c 20 2e 2e 2e 29 3c 2f   one call, ...)</
0380  61 3e 3c 62 72 2f 3e 0d 0a 2d 2d 3e 0d 0a 0d 0a   a><br/>..-->....
0390  09 3c 61 20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c   .<a href="./midl
03a0  65 74 73 2f 70 68 6f 74 6f 61 6c 62 75 6d 2e 6a   ets/photoalbum.j
03b0  61 64 22 3e 31 2e 2d 20 49 6d 61 67 65 73 20 44   ad">1.- Images D
03c0  65 6d 6f 3c 2f 61 3e 28 3c 61 20 68 72 65 66 3d   emo</a>(<a href=
03d0  22 2e 2f 69 6e 66 6f 2f 69 6d 61 67 65 5f 64 65   "./info/image_de
03e0  6d 6f 5f 69 6e 66 6f 2e 77 6d 6c 22 3e 69 6e 66   mo_info.wml">inf
03f0  6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c 61   o</a>)<br/>...<a
0400  20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74 73    href="./midlets
0410  2f 6d 6d 61 64 65 6d 6f 2e 6a 61 64 22 3e 32 2e   /mmademo.jad">2.
0420  2d 20 4d 4d 41 3c 2f 61 3e 28 3c 61 20 68 72 65   - MMA</a>(<a hre
0430  66 3d 22 2e 2f 69 6e 66 6f 2f 6d 6d 61 5f 64 65   f="./info/mma_de
0440  6d 6f 5f 69 6e 66 6f 2e 77 6d 6c 22 3e 69 6e 66   mo_info.wml">inf
0450  6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d 0a 09 3c 61   o</a>)<br/>...<a
0460  20 68 72 65 66 3d 22 2e 2f 6d 69 64 6c 65 74 73    href="./midlets
0470  2f 61 75 64 69 6f 64 65 6d 6f 2e 6a 61 64 22 3e   /audiodemo.jad">
0480  33 2e 2d 20 41 75 64 69 6f 3c 2f 61 3e 28 3c 61   3.- Audio</a>(<a
0490  20 68 72 65 66 3d 22 2e 2f 69 6e 66 6f 2f 61 75    href="./info/au
04a0  64 69 6f 5f 64 65 6d 6f 5f 69 6e 66 6f 2e 77 6d   dio_demo_info.wm
04b0  6c 22 3e 69 6e 66 6f 3c 2f 61 3e 29 3c 62 72 2f   l">info</a>)<br/
04c0  3e 0d 0a 09 3c 61 20 68 72 65 66 3d 22 2e 2f 6d   >...<a href="./m
04d0  69 64 6c 65 74 73 2f 53 4d 53 44 65 6d 6f 2e 6a   idlets/SMSDemo.j
04e0  61 64 22 3e 34 2e 2d 20 53 4d 53 3c 2f 61 3e 28   ad">4.- SMS</a>(
04f0  3c 61 20 68 72 65 66 3d 22 2e 2f 69 6e 66 6f 2f   <a href="./info/
0500  73 6d 73 5f 64 65 6d 6f 5f 69 6e 66 6f 2e 77 6d   sms_demo_info.wm
0510  6c 22 3e 69 6e 66 6f 3c 2f 61 3e 29 3c 62 72 2f   l">info</a>)<br/
0520  3e 0d 0a 09 3c 61 20 68 72 65 66 3d 22 2e 2f 6d   >...<a href="./m
0530  69 64 6c 65 74 73 2f 53 4d 53 50 75 73 68 44 65   idlets/SMSPushDe
0540  6d 6f 2e 6a 61 64 22 3e 35 2e 2d 20 53 4d 53 20   mo.jad">5.- SMS 
0550  50 55 53 48 3c 2f 61 3e 28 3c 61 20 68 72 65 66   PUSH</a>(<a href
0560  3d 22 2e 2f 69 6e 66 6f 2f 73 6d 73 5f 70 75 73   ="./info/sms_pus
0570  68 5f 64 65 6d 6f 5f 69 6e 66 6f 2e 77 6d 6c 22   h_demo_info.wml"
0580  3e 69 6e 66 6f 3c 2f 61 3e 29 3c 62 72 2f 3e 0d   >info</a>)<br/>.
0590  0a 09 3c 61 20 68 72 65 66 3d 22 2e 2f 6d 69 64   ..<a href="./mid
05a0  6c 65 74 73 2f 4e 65 74 77 6f 72 6b 44 65 6d 6f   lets/NetworkDemo
05b0  2e 6a 61 64 22 3e 36 2e 2d 20 4e 65 74 77 6f 72   .jad">6.- Networ
05c0  6b 3c 2f 61 3e 28 3c 61 20 68 72 65 66 3d 22 2e   k</a>(<a href=".
05d0  2f 69 6e 66 6f 2f 6e 65 74 77 6f 72 6b 5f 69 6e   /info/network_in
05e0  66 6f 2e 77 6d 6c 22 3e 69 6e                     fo.wml">in

Frame 54 (237 bytes on wire, 237 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.519690000
    Time delta from previous packet: 0.000013000 seconds
    Time since reference or first frame: 34.398341000 seconds
    Frame Number: 54
    Packet Length: 237 bytes
    Capture Length: 237 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 223
    Identification: 0x7589 (30089)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2de8)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48832 (48832), Seq: 1461, Ack: 738, Len: 183
    Source port: http (80)
    Destination port: 48832 (48832)
    Sequence number: 1461
    Next sequence number: 1644
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0018 (PSH, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 1... = Push: Set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x5779 (incorrect, should be 0x4266)
Hypertext Transfer Protocol
    Data (183 bytes)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 df 75 89 40 00 80 06 00 00 c3 eb a0 50 c3 37   ..u.@........P.7
0020  2f 34 00 50 be c0 7b 55 d2 c2 53 96 bb d3 50 18   /4.P..{U..S...P.
0030  41 8f 57 79 00 00 66 6f 3c 2f 61 3e 29 3c 62 72   A.Wy..fo</a>)<br
0040  2f 3e 0d 0a 3c 21 2d 2d 0d 0a 3c 61 20 68 72 65   />..<!--..<a hre
0050  66 3d 22 2e 2f 6d 69 64 6c 65 74 73 2f 42 6f 75   f="./midlets/Bou
0060  6e 63 65 2e 6a 61 64 22 3e 4d 49 44 6c 65 74 20   nce.jad">MIDlet 
0070  43 61 74 65 67 6f 72 79 3a 20 47 61 6d 65 73 3c   Category: Games<
0080  2f 61 3e 3c 62 72 2f 3e 0d 0a 3c 61 20 68 72 65   /a><br/>..<a hre
0090  66 3d 22 2e 2f 6d 69 64 6c 65 74 73 2f 48 61 77   f="./midlets/Haw
00a0  6b 2e 6a 61 64 22 3e 4d 49 44 6c 65 74 20 43 61   k.jad">MIDlet Ca
00b0  74 65 67 6f 72 79 3a 20 41 70 70 6c 69 63 61 74   tegory: Applicat
00c0  69 6f 6e 73 3c 2f 61 3e 3c 62 72 2f 3e 0d 0a 2d   ions</a><br/>..-
00d0  2d 3e 0d 0a 0d 0a 3c 2f 70 3e 0d 0a 0d 0a 3c 2f   ->....</p>....</
00e0  63 61 72 64 3e 0d 0a 3c 2f 77 6d 6c 3e            card>..</wml>

Frame 55 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.519736000
    Time delta from previous packet: 0.000046000 seconds
    Time since reference or first frame: 34.398387000 seconds
    Frame Number: 55
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x758a (30090)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2e9e)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48832 (48832), Seq: 1644, Ack: 738, Len: 0
    Source port: http (80)
    Destination port: 48832 (48832)
    Sequence number: 1644
    Acknowledgement number: 738
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 16783
    Checksum: 0x56c2 (incorrect, should be 0xfa52)

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 8a 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(u.@........P.7
0020  2f 34 00 50 be c0 7b 55 d3 79 53 96 bb d3 50 11   /4.P..{U.yS...P.
0030  41 8f 56 c2 00 00                                 A.V...

Frame 56 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.520408000
    Time delta from previous packet: 0.000672000 seconds
    Time since reference or first frame: 34.399059000 seconds
    Frame Number: 56
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x32ce (13006)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xb15a (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48832 (48832), Dst Port: http (80), Seq: 738, Ack: 1461, Len: 0
    Source port: 48832 (48832)
    Destination port: http (80)
    Sequence number: 738
    Acknowledgement number: 1461
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 7300
    Checksum: 0x2016 (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 53
        The RTT to ACK the segment was: 0.000731000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 32 ce 40 00 40 06 b1 5a c3 37 2f 34 c3 eb   .(2.@.@..Z.7/4..
0020  a0 50 be c0 00 50 53 96 bb d3 7b 55 d2 c2 50 10   .P...PS...{U..P.
0030  1c 84 20 16 00 00 00 00 00 00 00 00               .. .........

Frame 57 (60 bytes on wire, 60 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.541564000
    Time delta from previous packet: 0.021156000 seconds
    Time since reference or first frame: 34.420215000 seconds
    Frame Number: 57
    Packet Length: 60 bytes
    Capture Length: 60 bytes
Ethernet II, Src: 08:00:20:ec:0f:51, Dst: 00:0d:56:12:ab:7c
    Destination: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Source: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Type: IP (0x0800)
    Trailer: 000000000000
Internet Protocol, Src Addr: 195.55.47.52 (195.55.47.52), Dst Addr: marte (195.235.160.80)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x32cf (13007)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 64
    Protocol: TCP (0x06)
    Header checksum: 0xb159 (correct)
    Source: 195.55.47.52 (195.55.47.52)
    Destination: marte (195.235.160.80)
Transmission Control Protocol, Src Port: 48832 (48832), Dst Port: http (80), Seq: 738, Ack: 1645, Len: 0
    Source port: 48832 (48832)
    Destination port: http (80)
    Sequence number: 738
    Acknowledgement number: 1645
    Header length: 20 bytes
    Flags: 0x0011 (FIN, ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...1 = Fin: Set
    Window size: 7300
    Checksum: 0x1f5d (correct)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 55
        The RTT to ACK the segment was: 0.021828000 seconds

0000  00 0d 56 12 ab 7c 08 00 20 ec 0f 51 08 00 45 00   ..V..|.. ..Q..E.
0010  00 28 32 cf 40 00 40 06 b1 59 c3 37 2f 34 c3 eb   .(2.@.@..Y.7/4..
0020  a0 50 be c0 00 50 53 96 bb d3 7b 55 d3 7a 50 11   .P...PS...{U.zP.
0030  1c 84 1f 5d 00 00 00 00 00 00 00 00               ...]........

Frame 58 (54 bytes on wire, 54 bytes captured)
    Arrival Time: Apr 26, 2006 12:42:48.541573000
    Time delta from previous packet: 0.000009000 seconds
    Time since reference or first frame: 34.420224000 seconds
    Frame Number: 58
    Packet Length: 54 bytes
    Capture Length: 54 bytes
Ethernet II, Src: 00:0d:56:12:ab:7c, Dst: 08:00:20:ec:0f:51
    Destination: 08:00:20:ec:0f:51 (SunMicro_ec:0f:51)
    Source: 00:0d:56:12:ab:7c (DellPcba_12:ab:7c)
    Type: IP (0x0800)
Internet Protocol, Src Addr: marte (195.235.160.80), Dst Addr: 195.55.47.52 (195.55.47.52)
    Version: 4
    Header length: 20 bytes
    Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00)
        0000 00.. = Differentiated Services Codepoint: Default (0x00)
        .... ..0. = ECN-Capable Transport (ECT): 0
        .... ...0 = ECN-CE: 0
    Total Length: 40
    Identification: 0x758b (30091)
    Flags: 0x04
        .1.. = Don't fragment: Set
        ..0. = More fragments: Not set
    Fragment offset: 0
    Time to live: 128
    Protocol: TCP (0x06)
    Header checksum: 0x0000 (incorrect, should be 0x2e9d)
    Source: marte (195.235.160.80)
    Destination: 195.55.47.52 (195.55.47.52)
Transmission Control Protocol, Src Port: http (80), Dst Port: 48832 (48832), Seq: 1645, Ack: 739, Len: 0
    Source port: http (80)
    Destination port: 48832 (48832)
    Sequence number: 1645
    Acknowledgement number: 739
    Header length: 20 bytes
    Flags: 0x0010 (ACK)
        0... .... = Congestion Window Reduced (CWR): Not set
        .0.. .... = ECN-Echo: Not set
        ..0. .... = Urgent: Not set
        ...1 .... = Acknowledgment: Set
        .... 0... = Push: Not set
        .... .0.. = Reset: Not set
        .... ..0. = Syn: Not set
        .... ...0 = Fin: Not set
    Window size: 16783
    Checksum: 0x56c2 (incorrect, should be 0xfa51)
    SEQ/ACK analysis
        This is an ACK to the segment in frame: 57
        The RTT to ACK the segment was: 0.000009000 seconds

0000  08 00 20 ec 0f 51 00 0d 56 12 ab 7c 08 00 45 00   .. ..Q..V..|..E.
0010  00 28 75 8b 40 00 80 06 00 00 c3 eb a0 50 c3 37   .(u.@........P.7
0020  2f 34 00 50 be c0 7b 55 d3 7a 53 96 bb d4 50 10   /4.P..{U.zS...P.
0030  41 8f 56 c2 00 00                                 A.V...
